## Intersection of http://hl7.org/fhir/uv/ips/StructureDefinition/Device-observer-uv-ips and http://hl7.org/fhir/us/core/StructureDefinition/us-core-device

This is the set of resources that conform to both Device - Performer or Observer (IPS) (http://hl7.org/fhir/uv/ips/StructureDefinition/Device-observer-uv-ips) and US Core Device Profile (http://hl7.org/fhir/us/core/StructureDefinition/us-core-device).

### Structure

Name | Flags | Card. | Type | Description & Constraints Filter: Bindings Constraints Obligations
--- | --- | --- | --- | ---
Device |  | 0..* |  | Item used in healthcare
meta | Σ | 0..1 | Meta | Metadata about the resource
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: ?? (preferred): A human language.
Additional Bindings | Purpose
?? | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation This profile does not constrain the narrative in regard to content, language, or traceability to data elements
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
identifier | S | 0..* | Identifier | Instance identifier
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..1 | BackboneElement | left: Unique Device Identifier (UDI) Barcode string; right: 𝗔𝗗𝗗𝗜𝗧𝗜𝗢𝗡𝗔𝗟 𝗨𝗦𝗖𝗗𝗜: Unique Device Identifier (UDI) Barcode string
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | S Σ | 1..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | S Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: ?? (required): Codes to identify how UDI data was entered.
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: ?? (required): The availability status of the device.
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: ?? (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | left: The distinct identification string; right: 𝗔𝗗𝗗𝗜𝗧𝗜𝗢𝗡𝗔𝗟 𝗨𝗦𝗖𝗗𝗜: The distinct identification string
manufacturer | S | 0..1 | string | Name of device manufacturer
manufactureDate |  | 0..1 | dateTime | left: Date when the device was made; right: 𝗔𝗗𝗗𝗜𝗧𝗜𝗢𝗡𝗔𝗟 𝗨𝗦𝗖𝗗𝗜: Date when the device was made
expirationDate |  | 0..1 | dateTime | left: Date and time of expiry of this device (if applicable); right: 𝗔𝗗𝗗𝗜𝗧𝗜𝗢𝗡𝗔𝗟 𝗨𝗦𝗖𝗗𝗜: Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | left: Lot number of manufacture; right: 𝗔𝗗𝗗𝗜𝗧𝗜𝗢𝗡𝗔𝗟 𝗨𝗦𝗖𝗗𝗜: Lot number of manufacture
serialNumber |  | 0..1 | string | left: Serial number assigned by the manufacturer; right: 𝗔𝗗𝗗𝗜𝗧𝗜𝗢𝗡𝗔𝗟 𝗨𝗦𝗖𝗗𝗜: Serial number assigned by the manufacturer
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: ?? (required): The type of name the device is referred by.
modelNumber | S | 0..1 | string | The model number for the device
partNumber |  | 0..1 | string | The part number of the device
type | S | 1..1 | CodeableConcept | The kind or type of device Binding: ?? (extensible): Codes to identify medical devices
specialization |  | 0..* | BackboneElement | The capabilities supported on a device, the standards to which the device conforms for a particular purpose, and used for the communication
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The standard that is used to operate and communicate
version |  | 0..1 | string | The version of the standard that is used to operate and communicate
version |  | 0..* | BackboneElement | The actual design of the device or software version running on the device
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 0..1 | CodeableConcept | The type of the device version
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version text
property |  | 0..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
patient | S | 0..1 | Reference(http://hl7.org/fhir/us/core/StructureDefinition/us-core-patient) | left: Patient to whom Device is affixed; right: Patient to whom Device is assigned
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device
parent |  | 0..1 | Reference(Device) | The parent device
Documentation for this format