Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## : ASN1ToHL7 - TTL Representation

Raw ttl | Download

    @prefix fhir: <http://hl7.org/fhir/> .
    @prefix owl: <http://www.w3.org/2002/07/owl#> .
    @prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
    @prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

    # - resource -------------------------------------------------------------------

     a fhir:CodeSystem;
      fhir:nodeRole fhir:treeRoot;
      fhir:Resource.id [ fhir:value "ASN1ToHL7"];
      fhir:Resource.meta [
         fhir:Meta.profile [
           fhir:value "http://hl7.org/fhir/StructureDefinition/shareablecodesystem";
           fhir:index 0;
           fhir:link <http://hl7.org/fhir/StructureDefinition/shareablecodesystem>     ]
      ];
      fhir:DomainResource.text [
         fhir:Narrative.status [ fhir:value "generated" ];
         fhir:Narrative.div "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p><b>Properties</b></p><table class=\"grid\"><tr><td><b>Code</b></td><td><b>Type</b></td><td><b>Description</b></td></tr><tr><td>type</td><td>code</td><td>Indicates that the code type is an event or state</td></tr><tr><td>source</td><td>code</td><td>Indicates that the code originates from a measurement or an attribute that further describes a measurement or the sensor device.</td></tr></table><p>This code system http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7 defines the following codes:</p><table class=\"codes\"><tr><td><b>Lvl</b></td><td style=\"white-space:nowrap\"><b>Code</b></td><td><b>Display</b></td><td><b>Definition</b></td><td><b>type</b></td><td><b>source</b></td></tr><tr><td>1</td><td style=\"white-space:nowrap\">67925.0<a name=\"ASN1ToHL7-67925.460\"> </a></td><td>onMains</td><td>Indicates whether the PHD is on or off mains power</td><td>state</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">67925.1<a name=\"ASN1ToHL7-67925.461\"> </a></td><td>onBattery</td><td>Indicates whether the PHD is on or off Battery power</td><td>state</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">67925.8<a name=\"ASN1ToHL7-67925.468\"> </a></td><td>chargingFull</td><td>Indicates whether the PHD battery is charging at maximum rate</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">67925.9<a name=\"ASN1ToHL7-67925.469\"> </a></td><td>chargingTrickle</td><td>Indicates whether the PHD battery is charging at a trickle rate</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">67925.10<a name=\"ASN1ToHL7-67925.4610\"> </a></td><td>chargingOff</td><td>Indicates whether the PHD battery charging is on or off</td><td>state</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">532354.0<a name=\"ASN1ToHL7-532354.460\"> </a></td><td>regulation-status</td><td>Indicates device is regulated when cleared</td><td>state</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.0<a name=\"ASN1ToHL7-68219.460\"> </a></td><td>mds-time-capab-real-time-clock</td><td>Indicates real time clock is supported</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.1<a name=\"ASN1ToHL7-68219.461\"> </a></td><td>mds-time-capab-set-clock</td><td>Indicates support for the PHG to set the time</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.2<a name=\"ASN1ToHL7-68219.462\"> </a></td><td>mds-time-capab-relative-time</td><td>Indicates Relative Time is supported</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.3<a name=\"ASN1ToHL7-68219.463\"> </a></td><td>mds-time-capab-high-res-relative-time</td><td>Indicates Hi-Res Relative Time is supported</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.4<a name=\"ASN1ToHL7-68219.464\"> </a></td><td>mds-time-capab-sync-abs-time</td><td>Indicates that syncing the absolute time is supported</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.5<a name=\"ASN1ToHL7-68219.465\"> </a></td><td>mds-time-capab-sync-rel-time</td><td>Indicates that syncing the relative time is supported</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.6<a name=\"ASN1ToHL7-68219.466\"> </a></td><td>mds-time-capab-sync-hi-res-relative-time</td><td>Indicates that syncing hi-res relative time is supported</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.7<a name=\"ASN1ToHL7-68219.467\"> </a></td><td>mds-time-capab-bo-time</td><td>Indicates that the real-time clock supports base offset time</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.8<a name=\"ASN1ToHL7-68219.468\"> </a></td><td>mds-time-state-abs-time-synced</td><td>Indicates the absolute time has been synced</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.9<a name=\"ASN1ToHL7-68219.469\"> </a></td><td>mds-time-state-rel-time-synced</td><td>Indicates the relative time has been synced</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.10<a name=\"ASN1ToHL7-68219.4610\"> </a></td><td>mds-time-state-hi-res-relative-time-synced</td><td>Indicates the hi-res time has been synced</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.11<a name=\"ASN1ToHL7-68219.4611\"> </a></td><td>mds-time-mgr-set-time</td><td>PHG Requested to set the time</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.12<a name=\"ASN1ToHL7-68219.4612\"> </a></td><td>mds-time-capab-sync-bo-time</td><td>Indicates that syncing base-offset time is supported</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.13<a name=\"ASN1ToHL7-68219.4613\"> </a></td><td>mds-time-state-bo-time-synced</td><td>Indicates that base-offset time has been synced</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.14<a name=\"ASN1ToHL7-68219.4614\"> </a></td><td>mds-time-state-bo-time-UTC-aligned</td><td>Indicates that base-offset time is aligned with UTC time standard</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">68219.15<a name=\"ASN1ToHL7-68219.4615\"> </a></td><td>mds-time-dst-rules-enabled</td><td>Indicates support for daylight savings time rules</td><td>event</td><td>attribute</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">67846.0<a name=\"ASN1ToHL7-67846.460\"> </a></td><td>lim-alert-off</td><td>Indicates both the high and the low limit alerts are disabled</td><td>state</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">67846.1<a name=\"ASN1ToHL7-67846.461\"> </a></td><td>lim-low-off</td><td>Indicates the low limit alert is disabled</td><td>state</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">67846.2<a name=\"ASN1ToHL7-67846.462\"> </a></td><td>lim-high-off</td><td>Indicates the high limit alert is disabled</td><td>state</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.0<a name=\"ASN1ToHL7-150604.460\"> </a></td><td>sensor-disconnected</td><td>Indicates the device is not connected with the sensor</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.1<a name=\"ASN1ToHL7-150604.461\"> </a></td><td>sensor-malfunction</td><td>Indicates the sensor has malfunctioned</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.2<a name=\"ASN1ToHL7-150604.462\"> </a></td><td>sensor-displaced</td><td>Indicates the sensor is not correctly placed on the user</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.3<a name=\"ASN1ToHL7-150604.463\"> </a></td><td>sensor-unsupported</td><td>Indicates the sensor connected to the device is unsupported</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.4<a name=\"ASN1ToHL7-150604.464\"> </a></td><td>sensor-off</td><td>Indicates the sensor is not connected to the user</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.5<a name=\"ASN1ToHL7-150604.465\"> </a></td><td>sensor-interference</td><td>Indicates the sensor is experiencing interference</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.6<a name=\"ASN1ToHL7-150604.466\"> </a></td><td>signal-searching</td><td>Indicates the sensor is searching for a signal</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.7<a name=\"ASN1ToHL7-150604.467\"> </a></td><td>signal-pulse-questionable</td><td>Indicates a questionable pulse has been detected</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.8<a name=\"ASN1ToHL7-150604.468\"> </a></td><td>signal-non-pulsatile</td><td>Indicates a non pulsatile signal has been detected</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.9<a name=\"ASN1ToHL7-150604.469\"> </a></td><td>signal-erratic</td><td>Indicates a signal has been discovered, but it is erratic</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.10<a name=\"ASN1ToHL7-150604.4610\"> </a></td><td>signal-low-perfusion</td><td>Indicates the signal is experiencing low perfusion</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.11<a name=\"ASN1ToHL7-150604.4611\"> </a></td><td>signal-poor</td><td>Indicates the signal has been discovered, but it is poor</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.12<a name=\"ASN1ToHL7-150604.4612\"> </a></td><td>signal-inadequate</td><td>Indicates the signal has been discovered, but it is inadequate</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.13<a name=\"ASN1ToHL7-150604.4613\"> </a></td><td>signal-processing-irregularity</td><td>Indicates the signal has been discovered, but is experiencing processing irregularity</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.14<a name=\"ASN1ToHL7-150604.4614\"> </a></td><td>device-equipment-malfunction</td><td>Indicates a device malfunction has occurred</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150604.15<a name=\"ASN1ToHL7-150604.4615\"> </a></td><td>device-extended-update</td><td>Indicates an extended display update is in progress on device</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150605.0<a name=\"ASN1ToHL7-150605.460\"> </a></td><td>pulse-qual-nominal</td><td>Indicates no abnormalities have been detected by the sensor</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150605.1<a name=\"ASN1ToHL7-150605.461\"> </a></td><td>pulse-qual-marginal</td><td>Indicates the pulse profusion or quality is marginal</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150605.2<a name=\"ASN1ToHL7-150605.462\"> </a></td><td>pulse-qual-minimal</td><td>Indicates the pulse profusion or quality is minimal</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">150605.3<a name=\"ASN1ToHL7-150605.463\"> </a></td><td>pulse-qual-unacceptable</td><td>Indicates the pulse profusion or quality is unacceptable</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410584.0<a name=\"ASN1ToHL7-8410584.460\"> </a></td><td>leadwire-loss</td><td>Loss of unspecified lead wire or electrode connection</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410584.1<a name=\"ASN1ToHL7-8410584.461\"> </a></td><td>leadsignal-loss</td><td>Loss of unspecified lead signal</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410584.2<a name=\"ASN1ToHL7-8410584.462\"> </a></td><td>leadwire-loss-first-lead</td><td>Loss of 1st lead wire or electrode connection</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410584.3<a name=\"ASN1ToHL7-8410584.463\"> </a></td><td>leadsignal-loss-first-lead</td><td>Loss of 1st lead signal</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410584.4<a name=\"ASN1ToHL7-8410584.464\"> </a></td><td>leadwire-loss-second-lead</td><td>Loss of 2nd lead wire or electrode connection</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410584.5<a name=\"ASN1ToHL7-8410584.465\"> </a></td><td>leadsignal-loss-second-lead</td><td>Loss of 2nd lead signal</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410584.6<a name=\"ASN1ToHL7-8410584.466\"> </a></td><td>leadwire-loss-third-lead</td><td>Loss of 3rd lead wire or electrode connection</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410584.7<a name=\"ASN1ToHL7-8410584.467\"> </a></td><td>leadsignal-loss-third-lead</td><td>Loss of 3rd lead signal</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.0<a name=\"ASN1ToHL7-8417752.460\"> </a></td><td>device-battery-low</td><td>The device battery is low</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.1<a name=\"ASN1ToHL7-8417752.461\"> </a></td><td>sensor-malfunction</td><td>The sensor has malfunctioned</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.2<a name=\"ASN1ToHL7-8417752.462\"> </a></td><td>sensor-sample-size-insufficient</td><td>The sensor's sample size is insufficient</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.3<a name=\"ASN1ToHL7-8417752.463\"> </a></td><td>sensor-strip-insertion</td><td>The test strip was inserted incorrectly</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.4<a name=\"ASN1ToHL7-8417752.464\"> </a></td><td>sensor-strip-type-incorrect</td><td>The test strip type is incompatable with the sensor</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.5<a name=\"ASN1ToHL7-8417752.465\"> </a></td><td>sensor-result-too-high</td><td>The value reported by the sensor is too high</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.6<a name=\"ASN1ToHL7-8417752.466\"> </a></td><td>sensor-result-too-low</td><td>The value reported by the sensor is too low</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.7<a name=\"ASN1ToHL7-8417752.467\"> </a></td><td>sensor-temp-too-high</td><td>The temperature is too high</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.8<a name=\"ASN1ToHL7-8417752.468\"> </a></td><td>sensor-temp-too-low</td><td>The temperature is too low</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.9<a name=\"ASN1ToHL7-8417752.469\"> </a></td><td>sensor-read-interrupt</td><td>The read process was interrupted</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.10<a name=\"ASN1ToHL7-8417752.4610\"> </a></td><td>device-gen-fault</td><td>General Device Fault</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417752.11<a name=\"ASN1ToHL7-8417752.4611\"> </a></td><td>sensor-temp-out-of-range</td><td>The temperature is out of range</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.0<a name=\"ASN1ToHL7-8417909.460\"> </a></td><td>inr-device-battery-low</td><td>The INR device battery is low</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.1<a name=\"ASN1ToHL7-8417909.461\"> </a></td><td>inr-sensor-malfunction</td><td>The INR device sensor has malfunctioned</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.2<a name=\"ASN1ToHL7-8417909.462\"> </a></td><td>inr-sensor-sample-size-insufficient</td><td>The sample size was insufficient</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.3<a name=\"ASN1ToHL7-8417909.463\"> </a></td><td>inr-sensor-strip-insertion</td><td>The test script was inserted incorrectly</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.4<a name=\"ASN1ToHL7-8417909.464\"> </a></td><td>inr-sensor-strip-type-incorrect</td><td>The test strip used is not compatible with the INR</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.5<a name=\"ASN1ToHL7-8417909.465\"> </a></td><td>inr-sensor-result-too-high</td><td>The test result is too high</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.6<a name=\"ASN1ToHL7-8417909.466\"> </a></td><td>inr-sensor-result-too-low</td><td>The test result is too low</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.7<a name=\"ASN1ToHL7-8417909.467\"> </a></td><td>inr-sensor-temp-too-high</td><td>The temperature is too high</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.8<a name=\"ASN1ToHL7-8417909.468\"> </a></td><td>inr-sensor-temp-too-low</td><td>The temperature is too low</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.9<a name=\"ASN1ToHL7-8417909.469\"> </a></td><td>inr-sensor-read-interrupt</td><td>The read process was  interrupted</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.10<a name=\"ASN1ToHL7-8417909.4610\"> </a></td><td>inr-device-gen-fault</td><td>General device fault</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8417909.11<a name=\"ASN1ToHL7-8417909.4611\"> </a></td><td>inr-sensor-calibration-due</td><td>The INR sensor calibration is due</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.0<a name=\"ASN1ToHL7-8408608.460\"> </a></td><td>device-status-undetermined</td><td>Undetermined device status event</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.1<a name=\"ASN1ToHL7-8408608.461\"> </a></td><td>device-status-reset</td><td>Device reset</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.5<a name=\"ASN1ToHL7-8408608.465\"> </a></td><td>device-status-error</td><td>Device error</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.6<a name=\"ASN1ToHL7-8408608.466\"> </a></td><td>device-status-error-mechanical</td><td>Mechanical error</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.7<a name=\"ASN1ToHL7-8408608.467\"> </a></td><td>device-status-error-electronic</td><td>Electronic error</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.8<a name=\"ASN1ToHL7-8408608.468\"> </a></td><td>device-status-error-software</td><td>Software error</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.9<a name=\"ASN1ToHL7-8408608.469\"> </a></td><td>device-status-error-battery</td><td>Battery error</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.15<a name=\"ASN1ToHL7-8408608.4615\"> </a></td><td>device-status-service</td><td>Undetermined device status event, service needed</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.16<a name=\"ASN1ToHL7-8408608.4616\"> </a></td><td>device-status-service-time-sync-required</td><td>Time sync service required</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.17<a name=\"ASN1ToHL7-8408608.4617\"> </a></td><td>device-status-service-calibration-required</td><td>Calibration required</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.18<a name=\"ASN1ToHL7-8408608.4618\"> </a></td><td>device-status-service-replenishment-required</td><td>Replenishment required</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.25<a name=\"ASN1ToHL7-8408608.4625\"> </a></td><td>device-status-battery-low</td><td>Battery power is too low</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.26<a name=\"ASN1ToHL7-8408608.4626\"> </a></td><td>device-status-battery-depleted</td><td>Battery is depleted</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.27<a name=\"ASN1ToHL7-8408608.4627\"> </a></td><td>device-status-battery-replaced</td><td>Battery has been replaced</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8408608.28<a name=\"ASN1ToHL7-8408608.4628\"> </a></td><td>device-status-battery-interrupted</td><td>Battery was interrupted</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.0<a name=\"ASN1ToHL7-8418060.460\"> </a></td><td>sensor-session-stopped</td><td>Session stopped</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.2<a name=\"ASN1ToHL7-8418060.462\"> </a></td><td>sensor-type-incorrect</td><td>Sensor type incorrect for device</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.3<a name=\"ASN1ToHL7-8418060.463\"> </a></td><td>sensor-malfunction</td><td>The sensor malfunctioned</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.4<a name=\"ASN1ToHL7-8418060.464\"> </a></td><td>device-specific-alert</td><td>Device specific alert</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.7<a name=\"ASN1ToHL7-8418060.467\"> </a></td><td>sensor-calibration-not-allowed</td><td>Calibrating the sensor is not allowed</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.8<a name=\"ASN1ToHL7-8418060.468\"> </a></td><td>sensor-calibration-recommended</td><td>Calibrating the sensor is recommended</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.9<a name=\"ASN1ToHL7-8418060.469\"> </a></td><td>sensor-calibration-required</td><td>Calibrating the sensor is required</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.10<a name=\"ASN1ToHL7-8418060.4610\"> </a></td><td>sensor-temp-too-high</td><td>Temperature is too high for a valid result</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.11<a name=\"ASN1ToHL7-8418060.4611\"> </a></td><td>sensor-temp-too-low</td><td>Temperature is too low for a valid result</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.12<a name=\"ASN1ToHL7-8418060.4612\"> </a></td><td>sensor-result-below-patient-low</td><td>Sensor result below the Patient Low level</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.13<a name=\"ASN1ToHL7-8418060.4613\"> </a></td><td>sensor-result-above-patient-high</td><td>Sensor result above the Patient High level</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.14<a name=\"ASN1ToHL7-8418060.4614\"> </a></td><td>sensor-low-hypo</td><td>Sensor result below level</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.15<a name=\"ASN1ToHL7-8418060.4615\"> </a></td><td>sensor-high-hyper</td><td>Sensor result above level</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.16<a name=\"ASN1ToHL7-8418060.4616\"> </a></td><td>sensor-rate-decrease-exceeded</td><td>The sensor rate of decrease has been exceeded</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.17<a name=\"ASN1ToHL7-8418060.4617\"> </a></td><td>sensor-rate-increase-exceeded</td><td>The sensor rate of increase has been exceeded</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.18<a name=\"ASN1ToHL7-8418060.4618\"> </a></td><td>sensor-result-too-low</td><td>Sensor result is lower than the device can process</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.19<a name=\"ASN1ToHL7-8418060.4619\"> </a></td><td>sensor-result-too-high</td><td>Sensor result is higher than the device can process</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418060.20<a name=\"ASN1ToHL7-8418060.4620\"> </a></td><td>sensor-com-out-of-range</td><td>The sensor communication is out of range</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418512.0<a name=\"ASN1ToHL7-8418512.460\"> </a></td><td>Battery-status-Undetermined</td><td>the status of the battery is unknown</td><td>state</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418512.1<a name=\"ASN1ToHL7-8418512.461\"> </a></td><td>Battery-absent</td><td>Indicates if the battery is absent</td><td>state</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418512.2<a name=\"ASN1ToHL7-8418512.462\"> </a></td><td>Battery-active</td><td>Indicates if the battery is active in the system</td><td>state</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418512.3<a name=\"ASN1ToHL7-8418512.463\"> </a></td><td>Battery-charging</td><td>Indicates if the battery is charging</td><td>state</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418512.4<a name=\"ASN1ToHL7-8418512.464\"> </a></td><td>Battery-fullyCharged</td><td>Indicates if the battery is fully charged</td><td>state</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418512.5<a name=\"ASN1ToHL7-8418512.465\"> </a></td><td>Battery-disposable</td><td>Indicates if the battery is disposable</td><td>state</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418512.6<a name=\"ASN1ToHL7-8418512.466\"> </a></td><td>Battery-rechargeable</td><td>Indicates if battery is rechargable</td><td>state</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418512.8<a name=\"ASN1ToHL7-8418512.468\"> </a></td><td>Battery-faulty</td><td>Indicates if battery is faulty</td><td>event</td><td>measurement</td></tr><tr><td>2</td><td style=\"white-space:nowrap\">  8418512.7<a name=\"ASN1ToHL7-8418512.467\"> </a></td><td>Battery-overTemperature</td><td>Indicates if the battery is too hot</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8418512.9<a name=\"ASN1ToHL7-8418512.469\"> </a></td><td>Battery-incompatible</td><td>Indicates if battery is incompatible</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410608.0<a name=\"ASN1ToHL7-8410608.460\"> </a></td><td>body-movement</td><td>Indicates too much body movement</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410608.1<a name=\"ASN1ToHL7-8410608.461\"> </a></td><td>cuff-too-loose</td><td>Indicates the cuff was too loose</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410608.2<a name=\"ASN1ToHL7-8410608.462\"> </a></td><td>irregular-pulse</td><td>Indicates an irregular pulse was detected</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410608.3<a name=\"ASN1ToHL7-8410608.463\"> </a></td><td>pulse-over-range-limit</td><td>Indicates the pulse was too high for sensor to work</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410608.4<a name=\"ASN1ToHL7-8410608.464\"> </a></td><td>pulse-under-range-limit</td><td>Indicates the pulse was too low for sensor to work</td><td>event</td><td>measurement</td></tr><tr><td>1</td><td style=\"white-space:nowrap\">8410608.5<a name=\"ASN1ToHL7-8410608.465\"> </a></td><td>improper-body-position</td><td>Indicates the cuff was incorrectly placed with respect to the heart</td><td>event</td><td>measurement</td></tr></table></div>"
      ];
      fhir:CodeSystem.url [ fhir:value "http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7"];
      fhir:CodeSystem.version [ fhir:value "1.0.0"];
      fhir:CodeSystem.name [ fhir:value "ASN1ToHL7"];
      fhir:CodeSystem.status [ fhir:value "draft"];
      fhir:CodeSystem.experimental [ fhir:value "true"^^xsd:boolean];
      fhir:CodeSystem.date [ fhir:value "2018-09-18"^^xsd:date];
      fhir:CodeSystem.publisher [ fhir:value "HL7 International - Health Care Devices Work Group"];
      fhir:CodeSystem.contact [
         fhir:index 0;
         fhir:ContactDetail.telecom [
           fhir:index 0;
           fhir:ContactPoint.system [ fhir:value "url" ];
           fhir:ContactPoint.value [ fhir:value "http://hl7.org/Special/committees/healthcaredevices" ]     ]
      ];
      fhir:CodeSystem.description [ fhir:value "Maps IEEE 11073 ASN1 BITS measurements to codes. All these codes have two possible values, set or cleared. The code may either represent an event or a state. When an event, the defined event has occurred when set. If a state, the described item is either set or cleared. Sometimes the states may be defined in unexpected manners. For example, the regulation state when set is unregulated and when cleared it is regulated. In addition the code may derive from an IEEE 11073 attribute or from a measurement. More codes maybe added to this list in the future."];
      fhir:CodeSystem.jurisdiction [
         fhir:index 0;
         fhir:CodeableConcept.coding [
           fhir:index 0;
           fhir:Coding.system [ fhir:value "http://unstats.un.org/unsd/methods/m49/m49.htm" ];
           fhir:Coding.code [ fhir:value "001" ]     ]
      ];
      fhir:CodeSystem.caseSensitive [ fhir:value "true"^^xsd:boolean];
      fhir:CodeSystem.hierarchyMeaning [ fhir:value "grouped-by"];
      fhir:CodeSystem.content [ fhir:value "complete"];
      fhir:CodeSystem.property [
         fhir:index 0;
         fhir:CodeSystem.property.code [ fhir:value "type" ];
         fhir:CodeSystem.property.description [ fhir:value "Indicates that the code type is an event or state" ];
         fhir:CodeSystem.property.type [ fhir:value "code" ]
      ], [
         fhir:index 1;
         fhir:CodeSystem.property.code [ fhir:value "source" ];
         fhir:CodeSystem.property.description [ fhir:value "Indicates that the code originates from a measurement or an attribute that further describes a measurement or the sensor device." ];
         fhir:CodeSystem.property.type [ fhir:value "code" ]
      ];
      fhir:CodeSystem.concept [
         fhir:index 0;
         fhir:CodeSystem.concept.code [ fhir:value "67925.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "onMains" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates whether the PHD is on or off mains power" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 1;
         fhir:CodeSystem.concept.code [ fhir:value "67925.1" ];
         fhir:CodeSystem.concept.display [ fhir:value "onBattery" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates whether the PHD is on or off Battery power" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 2;
         fhir:CodeSystem.concept.code [ fhir:value "67925.8" ];
         fhir:CodeSystem.concept.display [ fhir:value "chargingFull" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates whether the PHD battery is charging at maximum rate" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 3;
         fhir:CodeSystem.concept.code [ fhir:value "67925.9" ];
         fhir:CodeSystem.concept.display [ fhir:value "chargingTrickle" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates whether the PHD battery is charging at a trickle rate" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 4;
         fhir:CodeSystem.concept.code [ fhir:value "67925.10" ];
         fhir:CodeSystem.concept.display [ fhir:value "chargingOff" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates whether the PHD battery charging is on or off" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 5;
         fhir:CodeSystem.concept.code [ fhir:value "532354.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "regulation-status" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates device is regulated when cleared" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 6;
         fhir:CodeSystem.concept.code [ fhir:value "68219.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-capab-real-time-clock" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates real time clock is supported" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 7;
         fhir:CodeSystem.concept.code [ fhir:value "68219.1" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-capab-set-clock" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates support for the PHG to set the time" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 8;
         fhir:CodeSystem.concept.code [ fhir:value "68219.2" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-capab-relative-time" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates Relative Time is supported" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 9;
         fhir:CodeSystem.concept.code [ fhir:value "68219.3" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-capab-high-res-relative-time" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates Hi-Res Relative Time is supported" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 10;
         fhir:CodeSystem.concept.code [ fhir:value "68219.4" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-capab-sync-abs-time" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates that syncing the absolute time is supported" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 11;
         fhir:CodeSystem.concept.code [ fhir:value "68219.5" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-capab-sync-rel-time" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates that syncing the relative time is supported" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 12;
         fhir:CodeSystem.concept.code [ fhir:value "68219.6" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-capab-sync-hi-res-relative-time" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates that syncing hi-res relative time is supported" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 13;
         fhir:CodeSystem.concept.code [ fhir:value "68219.7" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-capab-bo-time" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates that the real-time clock supports base offset time" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 14;
         fhir:CodeSystem.concept.code [ fhir:value "68219.8" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-state-abs-time-synced" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the absolute time has been synced" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 15;
         fhir:CodeSystem.concept.code [ fhir:value "68219.9" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-state-rel-time-synced" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the relative time has been synced" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 16;
         fhir:CodeSystem.concept.code [ fhir:value "68219.10" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-state-hi-res-relative-time-synced" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the hi-res time has been synced" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 17;
         fhir:CodeSystem.concept.code [ fhir:value "68219.11" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-mgr-set-time" ];
         fhir:CodeSystem.concept.definition [ fhir:value "PHG Requested to set the time" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 18;
         fhir:CodeSystem.concept.code [ fhir:value "68219.12" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-capab-sync-bo-time" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates that syncing base-offset time is supported" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 19;
         fhir:CodeSystem.concept.code [ fhir:value "68219.13" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-state-bo-time-synced" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates that base-offset time has been synced" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 20;
         fhir:CodeSystem.concept.code [ fhir:value "68219.14" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-state-bo-time-UTC-aligned" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates that base-offset time is aligned with UTC time standard" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 21;
         fhir:CodeSystem.concept.code [ fhir:value "68219.15" ];
         fhir:CodeSystem.concept.display [ fhir:value "mds-time-dst-rules-enabled" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates support for daylight savings time rules" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "attribute" ]     ]
      ], [
         fhir:index 22;
         fhir:CodeSystem.concept.code [ fhir:value "67846.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "lim-alert-off" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates both the high and the low limit alerts are disabled" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 23;
         fhir:CodeSystem.concept.code [ fhir:value "67846.1" ];
         fhir:CodeSystem.concept.display [ fhir:value "lim-low-off" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the low limit alert is disabled" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 24;
         fhir:CodeSystem.concept.code [ fhir:value "67846.2" ];
         fhir:CodeSystem.concept.display [ fhir:value "lim-high-off" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the high limit alert is disabled" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 25;
         fhir:CodeSystem.concept.code [ fhir:value "150604.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-disconnected" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the device is not connected with the sensor" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 26;
         fhir:CodeSystem.concept.code [ fhir:value "150604.1" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-malfunction" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the sensor has malfunctioned" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 27;
         fhir:CodeSystem.concept.code [ fhir:value "150604.2" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-displaced" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the sensor is not correctly placed on the user" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 28;
         fhir:CodeSystem.concept.code [ fhir:value "150604.3" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-unsupported" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the sensor connected to the device is unsupported" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 29;
         fhir:CodeSystem.concept.code [ fhir:value "150604.4" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-off" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the sensor is not connected to the user" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 30;
         fhir:CodeSystem.concept.code [ fhir:value "150604.5" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-interference" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the sensor is experiencing interference" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 31;
         fhir:CodeSystem.concept.code [ fhir:value "150604.6" ];
         fhir:CodeSystem.concept.display [ fhir:value "signal-searching" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the sensor is searching for a signal" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 32;
         fhir:CodeSystem.concept.code [ fhir:value "150604.7" ];
         fhir:CodeSystem.concept.display [ fhir:value "signal-pulse-questionable" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates a questionable pulse has been detected" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 33;
         fhir:CodeSystem.concept.code [ fhir:value "150604.8" ];
         fhir:CodeSystem.concept.display [ fhir:value "signal-non-pulsatile" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates a non pulsatile signal has been detected" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 34;
         fhir:CodeSystem.concept.code [ fhir:value "150604.9" ];
         fhir:CodeSystem.concept.display [ fhir:value "signal-erratic" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates a signal has been discovered, but it is erratic" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 35;
         fhir:CodeSystem.concept.code [ fhir:value "150604.10" ];
         fhir:CodeSystem.concept.display [ fhir:value "signal-low-perfusion" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the signal is experiencing low perfusion" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 36;
         fhir:CodeSystem.concept.code [ fhir:value "150604.11" ];
         fhir:CodeSystem.concept.display [ fhir:value "signal-poor" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the signal has been discovered, but it is poor" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 37;
         fhir:CodeSystem.concept.code [ fhir:value "150604.12" ];
         fhir:CodeSystem.concept.display [ fhir:value "signal-inadequate" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the signal has been discovered, but it is inadequate" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 38;
         fhir:CodeSystem.concept.code [ fhir:value "150604.13" ];
         fhir:CodeSystem.concept.display [ fhir:value "signal-processing-irregularity" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the signal has been discovered, but is experiencing processing irregularity" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 39;
         fhir:CodeSystem.concept.code [ fhir:value "150604.14" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-equipment-malfunction" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates a device malfunction has occurred" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 40;
         fhir:CodeSystem.concept.code [ fhir:value "150604.15" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-extended-update" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates an extended display update is in progress on device" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 41;
         fhir:CodeSystem.concept.code [ fhir:value "150605.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "pulse-qual-nominal" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates no abnormalities have been detected by the sensor" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 42;
         fhir:CodeSystem.concept.code [ fhir:value "150605.1" ];
         fhir:CodeSystem.concept.display [ fhir:value "pulse-qual-marginal" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the pulse profusion or quality is marginal" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 43;
         fhir:CodeSystem.concept.code [ fhir:value "150605.2" ];
         fhir:CodeSystem.concept.display [ fhir:value "pulse-qual-minimal" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the pulse profusion or quality is minimal" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 44;
         fhir:CodeSystem.concept.code [ fhir:value "150605.3" ];
         fhir:CodeSystem.concept.display [ fhir:value "pulse-qual-unacceptable" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the pulse profusion or quality is unacceptable" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 45;
         fhir:CodeSystem.concept.code [ fhir:value "8410584.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "leadwire-loss" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Loss of unspecified lead wire or electrode connection" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 46;
         fhir:CodeSystem.concept.code [ fhir:value "8410584.1" ];
         fhir:CodeSystem.concept.display [ fhir:value "leadsignal-loss" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Loss of unspecified lead signal" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 47;
         fhir:CodeSystem.concept.code [ fhir:value "8410584.2" ];
         fhir:CodeSystem.concept.display [ fhir:value "leadwire-loss-first-lead" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Loss of 1st lead wire or electrode connection" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 48;
         fhir:CodeSystem.concept.code [ fhir:value "8410584.3" ];
         fhir:CodeSystem.concept.display [ fhir:value "leadsignal-loss-first-lead" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Loss of 1st lead signal" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 49;
         fhir:CodeSystem.concept.code [ fhir:value "8410584.4" ];
         fhir:CodeSystem.concept.display [ fhir:value "leadwire-loss-second-lead" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Loss of 2nd lead wire or electrode connection" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 50;
         fhir:CodeSystem.concept.code [ fhir:value "8410584.5" ];
         fhir:CodeSystem.concept.display [ fhir:value "leadsignal-loss-second-lead" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Loss of 2nd lead signal" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 51;
         fhir:CodeSystem.concept.code [ fhir:value "8410584.6" ];
         fhir:CodeSystem.concept.display [ fhir:value "leadwire-loss-third-lead" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Loss of 3rd lead wire or electrode connection" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 52;
         fhir:CodeSystem.concept.code [ fhir:value "8410584.7" ];
         fhir:CodeSystem.concept.display [ fhir:value "leadsignal-loss-third-lead" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Loss of 3rd lead signal" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 53;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-battery-low" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The device battery is low" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 54;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.1" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-malfunction" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The sensor has malfunctioned" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 55;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.2" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-sample-size-insufficient" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The sensor's sample size is insufficient" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 56;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.3" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-strip-insertion" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The test strip was inserted incorrectly" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 57;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.4" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-strip-type-incorrect" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The test strip type is incompatable with the sensor" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 58;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.5" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-result-too-high" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The value reported by the sensor is too high" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 59;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.6" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-result-too-low" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The value reported by the sensor is too low" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 60;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.7" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-temp-too-high" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The temperature is too high" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 61;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.8" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-temp-too-low" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The temperature is too low" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 62;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.9" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-read-interrupt" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The read process was interrupted" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 63;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.10" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-gen-fault" ];
         fhir:CodeSystem.concept.definition [ fhir:value "General Device Fault" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 64;
         fhir:CodeSystem.concept.code [ fhir:value "8417752.11" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-temp-out-of-range" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The temperature is out of range" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 65;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-device-battery-low" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The INR device battery is low" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 66;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.1" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-sensor-malfunction" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The INR device sensor has malfunctioned" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 67;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.2" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-sensor-sample-size-insufficient" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The sample size was insufficient" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 68;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.3" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-sensor-strip-insertion" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The test script was inserted incorrectly" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 69;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.4" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-sensor-strip-type-incorrect" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The test strip used is not compatible with the INR" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 70;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.5" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-sensor-result-too-high" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The test result is too high" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 71;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.6" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-sensor-result-too-low" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The test result is too low" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 72;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.7" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-sensor-temp-too-high" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The temperature is too high" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 73;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.8" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-sensor-temp-too-low" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The temperature is too low" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 74;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.9" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-sensor-read-interrupt" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The read process was  interrupted" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 75;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.10" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-device-gen-fault" ];
         fhir:CodeSystem.concept.definition [ fhir:value "General device fault" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 76;
         fhir:CodeSystem.concept.code [ fhir:value "8417909.11" ];
         fhir:CodeSystem.concept.display [ fhir:value "inr-sensor-calibration-due" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The INR sensor calibration is due" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 77;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-undetermined" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Undetermined device status event" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 78;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.1" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-reset" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Device reset" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 79;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.5" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-error" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Device error" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 80;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.6" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-error-mechanical" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Mechanical error" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 81;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.7" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-error-electronic" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Electronic error" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 82;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.8" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-error-software" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Software error" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 83;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.9" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-error-battery" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Battery error" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 84;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.15" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-service" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Undetermined device status event, service needed" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 85;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.16" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-service-time-sync-required" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Time sync service required" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 86;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.17" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-service-calibration-required" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Calibration required" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 87;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.18" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-service-replenishment-required" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Replenishment required" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 88;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.25" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-battery-low" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Battery power is too low" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 89;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.26" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-battery-depleted" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Battery is depleted" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 90;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.27" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-battery-replaced" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Battery has been replaced" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 91;
         fhir:CodeSystem.concept.code [ fhir:value "8408608.28" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-status-battery-interrupted" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Battery was interrupted" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 92;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-session-stopped" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Session stopped" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 93;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.2" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-type-incorrect" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Sensor type incorrect for device" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 94;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.3" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-malfunction" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The sensor malfunctioned" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 95;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.4" ];
         fhir:CodeSystem.concept.display [ fhir:value "device-specific-alert" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Device specific alert" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 96;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.7" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-calibration-not-allowed" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Calibrating the sensor is not allowed" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 97;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.8" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-calibration-recommended" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Calibrating the sensor is recommended" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 98;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.9" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-calibration-required" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Calibrating the sensor is required" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 99;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.10" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-temp-too-high" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Temperature is too high for a valid result" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 100;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.11" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-temp-too-low" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Temperature is too low for a valid result" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 101;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.12" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-result-below-patient-low" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Sensor result below the Patient Low level" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 102;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.13" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-result-above-patient-high" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Sensor result above the Patient High level" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 103;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.14" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-low-hypo" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Sensor result below level" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 104;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.15" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-high-hyper" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Sensor result above level" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 105;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.16" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-rate-decrease-exceeded" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The sensor rate of decrease has been exceeded" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 106;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.17" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-rate-increase-exceeded" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The sensor rate of increase has been exceeded" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 107;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.18" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-result-too-low" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Sensor result is lower than the device can process" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 108;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.19" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-result-too-high" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Sensor result is higher than the device can process" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 109;
         fhir:CodeSystem.concept.code [ fhir:value "8418060.20" ];
         fhir:CodeSystem.concept.display [ fhir:value "sensor-com-out-of-range" ];
         fhir:CodeSystem.concept.definition [ fhir:value "The sensor communication is out of range" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 110;
         fhir:CodeSystem.concept.code [ fhir:value "8418512.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "Battery-status-Undetermined" ];
         fhir:CodeSystem.concept.definition [ fhir:value "the status of the battery is unknown" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 111;
         fhir:CodeSystem.concept.code [ fhir:value "8418512.1" ];
         fhir:CodeSystem.concept.display [ fhir:value "Battery-absent" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates if the battery is absent" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 112;
         fhir:CodeSystem.concept.code [ fhir:value "8418512.2" ];
         fhir:CodeSystem.concept.display [ fhir:value "Battery-active" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates if the battery is active in the system" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 113;
         fhir:CodeSystem.concept.code [ fhir:value "8418512.3" ];
         fhir:CodeSystem.concept.display [ fhir:value "Battery-charging" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates if the battery is charging" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 114;
         fhir:CodeSystem.concept.code [ fhir:value "8418512.4" ];
         fhir:CodeSystem.concept.display [ fhir:value "Battery-fullyCharged" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates if the battery is fully charged" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 115;
         fhir:CodeSystem.concept.code [ fhir:value "8418512.5" ];
         fhir:CodeSystem.concept.display [ fhir:value "Battery-disposable" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates if the battery is disposable" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 116;
         fhir:CodeSystem.concept.code [ fhir:value "8418512.6" ];
         fhir:CodeSystem.concept.display [ fhir:value "Battery-rechargeable" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates if battery is rechargable" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "state" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 117;
         fhir:CodeSystem.concept.code [ fhir:value "8418512.8" ];
         fhir:CodeSystem.concept.display [ fhir:value "Battery-faulty" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates if battery is faulty" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ];
         fhir:CodeSystem.concept.concept [
           fhir:index 0;
           fhir:CodeSystem.concept.code [ fhir:value "8418512.7" ];
           fhir:CodeSystem.concept.display [ fhir:value "Battery-overTemperature" ];
           fhir:CodeSystem.concept.definition [ fhir:value "Indicates if the battery is too hot" ];
           fhir:CodeSystem.concept.property [
             fhir:index 0;
             fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
             fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]       ], [
             fhir:index 1;
             fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
             fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]       ]     ]
      ], [
         fhir:index 118;
         fhir:CodeSystem.concept.code [ fhir:value "8418512.9" ];
         fhir:CodeSystem.concept.display [ fhir:value "Battery-incompatible" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates if battery is incompatible" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 119;
         fhir:CodeSystem.concept.code [ fhir:value "8410608.0" ];
         fhir:CodeSystem.concept.display [ fhir:value "body-movement" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates too much body movement" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 120;
         fhir:CodeSystem.concept.code [ fhir:value "8410608.1" ];
         fhir:CodeSystem.concept.display [ fhir:value "cuff-too-loose" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the cuff was too loose" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 121;
         fhir:CodeSystem.concept.code [ fhir:value "8410608.2" ];
         fhir:CodeSystem.concept.display [ fhir:value "irregular-pulse" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates an irregular pulse was detected" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 122;
         fhir:CodeSystem.concept.code [ fhir:value "8410608.3" ];
         fhir:CodeSystem.concept.display [ fhir:value "pulse-over-range-limit" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the pulse was too high for sensor to work" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 123;
         fhir:CodeSystem.concept.code [ fhir:value "8410608.4" ];
         fhir:CodeSystem.concept.display [ fhir:value "pulse-under-range-limit" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the pulse was too low for sensor to work" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ], [
         fhir:index 124;
         fhir:CodeSystem.concept.code [ fhir:value "8410608.5" ];
         fhir:CodeSystem.concept.display [ fhir:value "improper-body-position" ];
         fhir:CodeSystem.concept.definition [ fhir:value "Indicates the cuff was incorrectly placed with respect to the heart" ];
         fhir:CodeSystem.concept.property [
           fhir:index 0;
           fhir:CodeSystem.concept.property.code [ fhir:value "type" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "event" ]     ], [
           fhir:index 1;
           fhir:CodeSystem.concept.property.code [ fhir:value "source" ];
           fhir:CodeSystem.concept.property.valueString [ fhir:value "measurement" ]     ]
      ].

    # - ontology header ------------------------------------------------------------

     a owl:Ontology;
      owl:imports fhir:fhir.ttl.