Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## : Example of PHD Device - TTL Representation

Raw ttl | Download

    @prefix fhir: <http://hl7.org/fhir/> .
    @prefix owl: <http://www.w3.org/2002/07/owl#> .
    @prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
    @prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

    # - resource -------------------------------------------------------------------

     a fhir:Device;
      fhir:nodeRole fhir:treeRoot;
      fhir:Resource.id [ fhir:value "phd-74E8FFFEFF051C00.001C05FFE874"];
      fhir:Resource.meta [
         fhir:Meta.profile [
           fhir:value "http://hl7.org/fhir/uv/phd/StructureDefinition/PhdDevice";
           fhir:index 0;
           fhir:link <http://hl7.org/fhir/uv/phd/StructureDefinition/PhdDevice>     ]
      ];
      fhir:DomainResource.text [
         fhir:Narrative.status [ fhir:value "generated" ];
         fhir:Narrative.div "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p><b>Generated Narrative</b></p><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\">Resource \"phd-74E8FFFEFF051C00.001C05FFE874\" </p><p style=\"margin-bottom: 0px\">Profile: <a href=\"StructureDefinition-PhdDevice.html\">PhdDevice</a></p></div><p><b>identifier</b>: IEEE 11073 System Identifier: 74-E8-FF-FE-FF-05-1C-00, Bluetooth MAC address: 00-1C-05-FF-E8-74</p><p><b>manufacturer</b>: Nonin_Medical_Inc.</p><p><b>serialNumber</b>: 501900083</p><p><b>modelNumber</b>: Model 3230</p><p><b>type</b>: MDC_MOC_VMS_MDS_SIMP <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#65573)</span></p><h3>Specializations</h3><table class=\"grid\"><tr><td>-</td><td><b>SystemType</b></td><td><b>Version</b></td></tr><tr><td>*</td><td>MDC_DEV_SPEC_PROFILE_PULS_OXIM: Pulse Oximeter <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#528388)</span></td><td>1</td></tr></table><blockquote><p><b>version</b></p><p><b>type</b>: MDC_ID_PROD_SPEC_FW: Firmware revision <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#531976)</span></p><p><b>value</b>: r2.1</p></blockquote><blockquote><p><b>version</b></p><p><b>type</b>: MDC_ID_PROD_SPEC_SW: Software revision <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#531975)</span></p><p><b>value</b>: r1.5 9.7</p></blockquote><blockquote><p><b>version</b></p><p><b>type</b>: MDC_ID_PROD_SPEC_HW: Hardware revision <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#531974)</span></p><p><b>value</b>: r1.0</p></blockquote><blockquote><p><b>version</b></p><p><b>type</b>: MDC_REG_CERT_DATA_CONTINUA_VERSION: Continua version <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#532352)</span></p><p><b>value</b>: 6.0</p></blockquote><blockquote><p><b>property</b></p><p><b>type</b>: MDC_REG_CERT_DATA_CONTINUA_CERT_DEV_LIST: certified device list as transport-specialization combo <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#532353)</span></p><p><b>valueCode</b>: BTLE Pulse Oximeter certified <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"CodeSystem-ContinuaPHD.html\">ContinuaPHD</a>#32772)</span></p></blockquote><blockquote><p><b>property</b></p><p><b>type</b>: regulation-status <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"CodeSystem-ASN1ToHL7.html\">ASN1ToHL7</a>#532354.0)</span></p><p><b>valueCode</b>: Device is Regulated <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://hl7.org/fhir/R4/v2/0136/index.html\">v2 Y/N Indicator</a>#N)</span></p></blockquote><blockquote><p><b>property</b></p><p><b>type</b>: MDC_TIME_SYNC_PROTOCOL: Time synchronization protocol <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#68220)</span></p><p><b>valueCode</b>: MDC_TIME_SYNC_NONE: <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#532224)</span></p></blockquote></div>"
      ];
      fhir:Device.identifier [
         fhir:index 0;
         fhir:Identifier.type [
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers" ];
             fhir:Coding.code [ fhir:value "SYSID" ]       ]     ];
         fhir:Identifier.system [ fhir:value "urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680" ];
         fhir:Identifier.value [ fhir:value "74-E8-FF-FE-FF-05-1C-00" ]
      ], [
         fhir:index 1;
         fhir:Identifier.type [
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers" ];
             fhir:Coding.code [ fhir:value "BTMAC" ]       ]     ];
         fhir:Identifier.system [ fhir:value "http://hl7.org/fhir/sid/eui-48/bluetooth" ];
         fhir:Identifier.value [ fhir:value "00-1C-05-FF-E8-74" ]
      ];
      fhir:Device.manufacturer [ fhir:value "Nonin_Medical_Inc."];
      fhir:Device.serialNumber [ fhir:value "501900083"];
      fhir:Device.modelNumber [ fhir:value "Model 3230"];
      fhir:Device.type [
         fhir:CodeableConcept.coding [
           fhir:index 0;
           fhir:Coding.system [ fhir:value "urn:iso:std:iso:11073:10101" ];
           fhir:Coding.code [ fhir:value "65573" ]     ];
         fhir:CodeableConcept.text [ fhir:value "MDC_MOC_VMS_MDS_SIMP" ]
      ];
      fhir:Device.specialization [
         fhir:index 0;
         fhir:Device.specialization.systemType [
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "urn:iso:std:iso:11073:10101" ];
             fhir:Coding.code [ fhir:value "528388" ]       ];
           fhir:CodeableConcept.text [ fhir:value "MDC_DEV_SPEC_PROFILE_PULS_OXIM: Pulse Oximeter" ]     ];
         fhir:Device.specialization.version [ fhir:value "1" ]
      ];
      fhir:Device.version [
         fhir:index 0;
         fhir:Device.version.type [
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "urn:iso:std:iso:11073:10101" ];
             fhir:Coding.code [ fhir:value "531976" ]       ];
           fhir:CodeableConcept.text [ fhir:value "MDC_ID_PROD_SPEC_FW: Firmware revision" ]     ];
         fhir:Device.version.value [ fhir:value "r2.1" ]
      ], [
         fhir:index 1;
         fhir:Device.version.type [
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "urn:iso:std:iso:11073:10101" ];
             fhir:Coding.code [ fhir:value "531975" ]       ];
           fhir:CodeableConcept.text [ fhir:value "MDC_ID_PROD_SPEC_SW: Software revision" ]     ];
         fhir:Device.version.value [ fhir:value "r1.5 9.7" ]
      ], [
         fhir:index 2;
         fhir:Device.version.type [
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "urn:iso:std:iso:11073:10101" ];
             fhir:Coding.code [ fhir:value "531974" ]       ];
           fhir:CodeableConcept.text [ fhir:value "MDC_ID_PROD_SPEC_HW: Hardware revision" ]     ];
         fhir:Device.version.value [ fhir:value "r1.0" ]
      ], [
         fhir:index 3;
         fhir:Device.version.type [
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "urn:iso:std:iso:11073:10101" ];
             fhir:Coding.code [ fhir:value "532352" ]       ];
           fhir:CodeableConcept.text [ fhir:value "MDC_REG_CERT_DATA_CONTINUA_VERSION: Continua version" ]     ];
         fhir:Device.version.value [ fhir:value "6.0" ]
      ];
      fhir:Device.property [
         fhir:index 0;
         fhir:Device.property.type [
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "urn:iso:std:iso:11073:10101" ];
             fhir:Coding.code [ fhir:value "532353" ]       ];
           fhir:CodeableConcept.text [ fhir:value "MDC_REG_CERT_DATA_CONTINUA_CERT_DEV_LIST: certified device list as transport-specialization combo" ]     ];
         fhir:Device.property.valueCode [
           fhir:index 0;
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaPHD" ];
             fhir:Coding.code [ fhir:value "32772" ]       ]     ]
      ], [
         fhir:index 1;
         fhir:Device.property.type [
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7" ];
             fhir:Coding.code [ fhir:value "532354.0" ]       ];
           fhir:CodeableConcept.text [ fhir:value "regulation-status" ]     ];
         fhir:Device.property.valueCode [
           fhir:index 0;
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "http://terminology.hl7.org/CodeSystem/v2-0136" ];
             fhir:Coding.code [ fhir:value "N" ]       ];
           fhir:CodeableConcept.text [ fhir:value "Device is Regulated" ]     ]
      ], [
         fhir:index 2;
         fhir:Device.property.type [
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "urn:iso:std:iso:11073:10101" ];
             fhir:Coding.code [ fhir:value "68220" ]       ];
           fhir:CodeableConcept.text [ fhir:value "MDC_TIME_SYNC_PROTOCOL: Time synchronization protocol" ]     ];
         fhir:Device.property.valueCode [
           fhir:index 0;
           fhir:CodeableConcept.coding [
             fhir:index 0;
             fhir:Coding.system [ fhir:value "urn:iso:std:iso:11073:10101" ];
             fhir:Coding.code [ fhir:value "532224" ]       ];
           fhir:CodeableConcept.text [ fhir:value "MDC_TIME_SYNC_NONE:" ]     ]
      ].

    # - ontology header ------------------------------------------------------------

     a owl:Ontology;
      owl:imports fhir:fhir.ttl.