Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## : ContinuaDeviceIdentifiers - TTL Representation

Raw ttl | Download

    @prefix fhir: <http://hl7.org/fhir/> .
    @prefix owl: <http://www.w3.org/2002/07/owl#> .
    @prefix rdfs: <http://www.w3.org/2000/01/rdf-schema#> .
    @prefix xsd: <http://www.w3.org/2001/XMLSchema#> .

    # - resource -------------------------------------------------------------------

     a fhir:CodeSystem;
      fhir:nodeRole fhir:treeRoot;
      fhir:Resource.id [ fhir:value "ContinuaDeviceIdentifiers"];
      fhir:Resource.meta [
         fhir:Meta.profile [
           fhir:value "http://hl7.org/fhir/StructureDefinition/shareablecodesystem";
           fhir:index 0;
           fhir:link <http://hl7.org/fhir/StructureDefinition/shareablecodesystem>     ]
      ];
      fhir:DomainResource.text [
         fhir:Narrative.status [ fhir:value "generated" ];
         fhir:Narrative.div "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p>This code system http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers defines the following codes:</p><table class=\"codes\"><tr><td style=\"white-space:nowrap\"><b>Code</b></td><td><b>Display</b></td><td><b>Definition</b></td></tr><tr><td style=\"white-space:nowrap\">SYSID<a name=\"ContinuaDeviceIdentifiers-SYSID\"> </a></td><td>IEEE 11073 System Identifier</td><td>This code indicates that the identifier is the IEEE 11073 SystemId from the equivalent of the System-Id attribute</td></tr><tr><td style=\"white-space:nowrap\">BTMAC<a name=\"ContinuaDeviceIdentifiers-BTMAC\"> </a></td><td>Bluetooth MAC address</td><td>This code indicates that the identifier is the Bluetooth MAC address, either classic or low energy</td></tr><tr><td style=\"white-space:nowrap\">ETHMAC<a name=\"ContinuaDeviceIdentifiers-ETHMAC\"> </a></td><td>Ethernet MAC address</td><td>This code indicates that the identifier is the Ethernet MAC address</td></tr><tr><td style=\"white-space:nowrap\">USB<a name=\"ContinuaDeviceIdentifiers-USB\"> </a></td><td>USB PID and VID designators</td><td>This code indicates that the identifier is the USB Pid and Vid values</td></tr><tr><td style=\"white-space:nowrap\">ZIGBEE<a name=\"ContinuaDeviceIdentifiers-ZIGBEE\"> </a></td><td>ZigBee MAC address</td><td>This code indicates that the identifier is the ZigBee MAC address</td></tr></table></div>"
      ];
      fhir:CodeSystem.url [ fhir:value "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers"];
      fhir:CodeSystem.version [ fhir:value "1.0.0"];
      fhir:CodeSystem.name [ fhir:value "ContinuaDeviceIdentifiers"];
      fhir:CodeSystem.status [ fhir:value "draft"];
      fhir:CodeSystem.experimental [ fhir:value "true"^^xsd:boolean];
      fhir:CodeSystem.date [ fhir:value "2018-11-25"^^xsd:date];
      fhir:CodeSystem.publisher [ fhir:value "HL7 International - Health Care Devices Work Group"];
      fhir:CodeSystem.contact [
         fhir:index 0;
         fhir:ContactDetail.telecom [
           fhir:index 0;
           fhir:ContactPoint.system [ fhir:value "url" ];
           fhir:ContactPoint.value [ fhir:value "http://hl7.org/Special/committees/healthcaredevices" ]     ]
      ];
      fhir:CodeSystem.description [ fhir:value "Codes used to describe the Device (PHD or PHG) Identifiers, such as the system id or Bluetooth Address. More codes maybe added to this list in the future."];
      fhir:CodeSystem.jurisdiction [
         fhir:index 0;
         fhir:CodeableConcept.coding [
           fhir:index 0;
           fhir:Coding.system [ fhir:value "http://unstats.un.org/unsd/methods/m49/m49.htm" ];
           fhir:Coding.code [ fhir:value "001" ]     ]
      ];
      fhir:CodeSystem.caseSensitive [ fhir:value "true"^^xsd:boolean];
      fhir:CodeSystem.hierarchyMeaning [ fhir:value "grouped-by"];
      fhir:CodeSystem.content [ fhir:value "complete"];
      fhir:CodeSystem.concept [
         fhir:index 0;
         fhir:CodeSystem.concept.code [ fhir:value "SYSID" ];
         fhir:CodeSystem.concept.display [ fhir:value "IEEE 11073 System Identifier" ];
         fhir:CodeSystem.concept.definition [ fhir:value "This code indicates that the identifier is the IEEE 11073 SystemId from the equivalent of the System-Id attribute" ]
      ], [
         fhir:index 1;
         fhir:CodeSystem.concept.code [ fhir:value "BTMAC" ];
         fhir:CodeSystem.concept.display [ fhir:value "Bluetooth MAC address" ];
         fhir:CodeSystem.concept.definition [ fhir:value "This code indicates that the identifier is the Bluetooth MAC address, either classic or low energy" ]
      ], [
         fhir:index 2;
         fhir:CodeSystem.concept.code [ fhir:value "ETHMAC" ];
         fhir:CodeSystem.concept.display [ fhir:value "Ethernet MAC address" ];
         fhir:CodeSystem.concept.definition [ fhir:value "This code indicates that the identifier is the Ethernet MAC address" ]
      ], [
         fhir:index 3;
         fhir:CodeSystem.concept.code [ fhir:value "USB" ];
         fhir:CodeSystem.concept.display [ fhir:value "USB PID and VID designators" ];
         fhir:CodeSystem.concept.definition [ fhir:value "This code indicates that the identifier is the USB Pid and Vid values" ]
      ], [
         fhir:index 4;
         fhir:CodeSystem.concept.code [ fhir:value "ZIGBEE" ];
         fhir:CodeSystem.concept.display [ fhir:value "ZigBee MAC address" ];
         fhir:CodeSystem.concept.definition [ fhir:value "This code indicates that the identifier is the ZigBee MAC address" ]
      ].

    # - ontology header ------------------------------------------------------------

     a owl:Ontology;
      owl:imports fhir:fhir.ttl.