Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## Example Observation: Example of a ASN1 BITs measurement

Generated Narrative

Resource "bits-1.0.0.40"

Profile: PhdBitsEnumerationObservation

Gateway Device: Device/phg-ecde3d4e58532d31.000000000000

status: final

code: MDC_PULS_OXIM_DEV_STATUS: Measuring process issues (ISO 11073-10101 Health informatics - Point-of-care#150604)

subject: Patient/sisansarahId.1.2.3.4.5.6.7.8.10 " PIGGY"

effective: 2018-11-11 07:07:48-0500

device: Device/phd-74E8FFFEFF051C00.001C05FFE874

> component

> code: sensor-displaced (ASN1ToHL7#150604.2)

> value: Sensor is incorrectly placed on user (v2 Y/N Indicator#Y)

> component

> code: signal-pulse-questionable (ASN1ToHL7#150604.7)

> value: Questionable pulse detected (v2 Y/N Indicator#Y)

> component

> code: signal-low-perfusion (ASN1ToHL7#150604.10)

> value: Signal experiencing low perfusion (v2 Y/N Indicator#Y)

> component

> code: signal-poor (ASN1ToHL7#150604.11)

> value: Signal is poor (v2 Y/N Indicator#Y)

> component

> code: signal-inadequate (ASN1ToHL7#150604.12)

> value: Signal is inadequate (v2 Y/N Indicator#Y)