Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## : ContinuaDeviceIdentifiers - XML Representation

Raw xml | Download

    <CodeSystem xmlns="http://hl7.org/fhir">
      <id value="ContinuaDeviceIdentifiers"/>
      <meta>
        <profile value="http://hl7.org/fhir/StructureDefinition/shareablecodesystem"/>
      </meta>
      <text>
        <status value="generated"/>
        <div xmlns="http://www.w3.org/1999/xhtml"><p>This code system http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers defines the following codes:</p><table class="codes"><tr><td style="white-space:nowrap"><b>Code</b></td><td><b>Display</b></td><td><b>Definition</b></td></tr><tr><td style="white-space:nowrap">SYSID<a name="ContinuaDeviceIdentifiers-SYSID"> </a></td><td>IEEE 11073 System Identifier</td><td>This code indicates that the identifier is the IEEE 11073 SystemId from the equivalent of the System-Id attribute</td></tr><tr><td style="white-space:nowrap">BTMAC<a name="ContinuaDeviceIdentifiers-BTMAC"> </a></td><td>Bluetooth MAC address</td><td>This code indicates that the identifier is the Bluetooth MAC address, either classic or low energy</td></tr><tr><td style="white-space:nowrap">ETHMAC<a name="ContinuaDeviceIdentifiers-ETHMAC"> </a></td><td>Ethernet MAC address</td><td>This code indicates that the identifier is the Ethernet MAC address</td></tr><tr><td style="white-space:nowrap">USB<a name="ContinuaDeviceIdentifiers-USB"> </a></td><td>USB PID and VID designators</td><td>This code indicates that the identifier is the USB Pid and Vid values</td></tr><tr><td style="white-space:nowrap">ZIGBEE<a name="ContinuaDeviceIdentifiers-ZIGBEE"> </a></td><td>ZigBee MAC address</td><td>This code indicates that the identifier is the ZigBee MAC address</td></tr></table></div>
      </text>
      <url value="http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers"/>
      <version value="1.0.0"/>
      <name value="ContinuaDeviceIdentifiers"/>
      <status value="draft"/>
      <experimental value="true"/>
      <date value="2018-11-25"/>
      <publisher value="HL7 International - Health Care Devices Work Group"/>
      <contact>
        <telecom>
          <system value="url"/>
          <value value="http://hl7.org/Special/committees/healthcaredevices"/>
        </telecom>
      </contact>
      <description
                   value="Codes used to describe the Device (PHD or PHG) Identifiers, such as the system id or Bluetooth Address. More codes maybe added to this list in the future."/>
      <jurisdiction>
        <coding>
          <system value="http://unstats.un.org/unsd/methods/m49/m49.htm"/>
          <code value="001"/>
        </coding>
      </jurisdiction>
      <caseSensitive value="true"/>
      <hierarchyMeaning value="grouped-by"/>
      <content value="complete"/>
      <concept>
        <code value="SYSID"/>
        <display value="IEEE 11073 System Identifier"/>
        <definition
                    value="This code indicates that the identifier is the IEEE 11073 SystemId from the equivalent of the System-Id attribute"/>
      </concept>
      <concept>
        <code value="BTMAC"/>
        <display value="Bluetooth MAC address"/>
        <definition
                    value="This code indicates that the identifier is the Bluetooth MAC address, either classic or low energy"/>
      </concept>
      <concept>
        <code value="ETHMAC"/>
        <display value="Ethernet MAC address"/>
        <definition
                    value="This code indicates that the identifier is the Ethernet MAC address"/>
      </concept>
      <concept>
        <code value="USB"/>
        <display value="USB PID and VID designators"/>
        <definition
                    value="This code indicates that the identifier is the USB Pid and Vid values"/>
      </concept>
      <concept>
        <code value="ZIGBEE"/>
        <display value="ZigBee MAC address"/>
        <definition
                    value="This code indicates that the identifier is the ZigBee MAC address"/>
      </concept>
    </CodeSystem>