## CodeSystem Comparison between http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7 vs http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7

### Messages

Error | CodeSystem.version | Values for version differ: '0.3.0' vs '1.0.0'
Information | CodeSystem.date | Values for date differ: '2018-09-18T00:00:00+10:00' vs '2018-09-18'
Information | CodeSystem.publisher | Values for publisher differ: 'Health Level Seven International (Health Care Devices Work Group)' vs 'HL7 International - Health Care Devices Work Group'
Information | CodeSystem.jurisdiction | Added the item 'http://unstats.un.org/unsd/methods/m49/m49.htm#001'
Warning | CodeSystem.concept.where(code='67925.0').display | Changed value for display: 'Mains power state' vs 'onMains'
Warning | CodeSystem.concept.where(code='67925.1').display | Changed value for display: 'Battery state' vs 'onBattery'
Warning | CodeSystem.concept.where(code='67925.8').display | Changed value for display: 'Charging at full rate' vs 'chargingFull'
Warning | CodeSystem.concept.where(code='67925.9').display | Changed value for display: 'Charging at trickle rate' vs 'chargingTrickle'
Warning | CodeSystem.concept.where(code='67925.10').display | Changed value for display: 'Charging state' vs 'chargingOff'
Warning | CodeSystem.concept.where(code='532354.0').display | Changed value for display: 'If bit is cleared device is regulated' vs 'regulation-status'
Information | CodeSystem.concept.where(code='532354.0').definition | Changed value for definition: 'Indicates whether the device is regulated' vs 'Indicates device is regulated when cleared'
Warning | CodeSystem.concept.where(code='68219.0').display | Changed value for display: 'Real-time clock' vs 'mds-time-capab-real-time-clock'
Warning | CodeSystem.concept.where(code='68219.1').display | Changed value for display: 'PHG set-time' vs 'mds-time-capab-set-clock'
Warning | CodeSystem.concept.where(code='68219.2').display | Changed value for display: 'Relative Time' vs 'mds-time-capab-relative-time'
Warning | CodeSystem.concept.where(code='68219.3').display | Changed value for display: 'Hi-Res Relative Time' vs 'mds-time-capab-high-res-relative-time'
Warning | CodeSystem.concept.where(code='68219.4').display | Changed value for display: 'Sync Absolute Time' vs 'mds-time-capab-sync-abs-time'
Warning | CodeSystem.concept.where(code='68219.5').display | Changed value for display: 'Sync Relative Time' vs 'mds-time-capab-sync-rel-time'
Warning | CodeSystem.concept.where(code='68219.6').display | Changed value for display: 'Sync Hi-Res Relative Time' vs 'mds-time-capab-sync-hi-res-relative-time'
Warning | CodeSystem.concept.where(code='68219.7').display | Changed value for display: 'Base Offset Time' vs 'mds-time-capab-bo-time'
Warning | CodeSystem.concept.where(code='68219.8').display | Changed value for display: 'Absolute Time Synced' vs 'mds-time-state-abs-time-synced'
Warning | CodeSystem.concept.where(code='68219.9').display | Changed value for display: 'Relative Time Synced' vs 'mds-time-state-rel-time-synced'
Warning | CodeSystem.concept.where(code='68219.10').display | Changed value for display: 'Hi-Res Relative Time Synced' vs 'mds-time-state-hi-res-relative-time-synced'
Warning | CodeSystem.concept.where(code='68219.11').display | Changed value for display: 'PHG Set-Time Requested' vs 'mds-time-mgr-set-time'
Warning | CodeSystem.concept.where(code='68219.12').display | Changed value for display: 'Syncing base-offset time support' vs 'mds-time-capab-sync-bo-time'
Warning | CodeSystem.concept.where(code='68219.13').display | Changed value for display: 'Base-Offset Time Synced' vs 'mds-time-state-bo-time-synced'
Warning | CodeSystem.concept.where(code='68219.14').display | Changed value for display: 'Base-Offset Time UTC Aligned' vs 'mds-time-state-bo-time-UTC-aligned'
Warning | CodeSystem.concept.where(code='68219.15').display | Changed value for display: 'Daylight Savings Time Rules Understood' vs 'mds-time-dst-rules-enabled'
Warning | CodeSystem.concept.where(code='67846.0').display | Changed value for display: 'All alerts disabled' vs 'lim-alert-off'
Warning | CodeSystem.concept.where(code='67846.1').display | Changed value for display: 'Low limit alert disabled' vs 'lim-low-off'
Warning | CodeSystem.concept.where(code='67846.2').display | Changed value for display: 'High limit alert disabled' vs 'lim-high-off'
Warning | CodeSystem.concept.where(code='150604.0').display | Changed value for display: 'Device not connected to sensor' vs 'sensor-disconnected'
Warning | CodeSystem.concept.where(code='150604.1').display | Changed value for display: 'Sensor has malfunctioned' vs 'sensor-malfunction'
Warning | CodeSystem.concept.where(code='150604.2').display | Changed value for display: 'Sensor incorrectly placed on user' vs 'sensor-displaced'
Warning | CodeSystem.concept.where(code='150604.3').display | Changed value for display: 'Unsupported sensor' vs 'sensor-unsupported'
Warning | CodeSystem.concept.where(code='150604.4').display | Changed value for display: 'Sensor off' vs 'sensor-off'
Warning | CodeSystem.concept.where(code='150604.5').display | Changed value for display: 'Sensor interference' vs 'sensor-interference'
Warning | CodeSystem.concept.where(code='150604.6').display | Changed value for display: 'Searching for signal' vs 'signal-searching'
Warning | CodeSystem.concept.where(code='150604.7').display | Changed value for display: 'Signal pulse questionable' vs 'signal-pulse-questionable'
Warning | CodeSystem.concept.where(code='150604.8').display | Changed value for display: 'Non pulsatile signal' vs 'signal-non-pulsatile'
Warning | CodeSystem.concept.where(code='150604.9').display | Changed value for display: 'Signal erratic' vs 'signal-erratic'
Warning | CodeSystem.concept.where(code='150604.10').display | Changed value for display: 'Signal low perfusion' vs 'signal-low-perfusion'
Warning | CodeSystem.concept.where(code='150604.11').display | Changed value for display: 'Signal is poor' vs 'signal-poor'
Warning | CodeSystem.concept.where(code='150604.12').display | Changed value for display: 'Signal inadequate' vs 'signal-inadequate'
Warning | CodeSystem.concept.where(code='150604.13').display | Changed value for display: 'Signal experiencing processing irregularity' vs 'signal-processing-irregularity'
Warning | CodeSystem.concept.where(code='150604.14').display | Changed value for display: 'Device malfunction' vs 'device-equipment-malfunction'
Warning | CodeSystem.concept.where(code='150604.15').display | Changed value for display: 'Device extended update' vs 'device-extended-update'
Warning | CodeSystem.concept.where(code='150605.0').display | Changed value for display: 'Pulse quality nominal' vs 'pulse-qual-nominal'
Warning | CodeSystem.concept.where(code='150605.1').display | Changed value for display: 'Pulse quality marginal' vs 'pulse-qual-marginal'
Warning | CodeSystem.concept.where(code='150605.2').display | Changed value for display: 'Pulse quality minimal' vs 'pulse-qual-minimal'
Warning | CodeSystem.concept.where(code='150605.3').display | Changed value for display: 'Pulse quality unacceptable' vs 'pulse-qual-unacceptable'
Warning | CodeSystem.concept.where(code='8410584.0').display | Changed value for display: 'Lead wire loss' vs 'leadwire-loss'
Warning | CodeSystem.concept.where(code='8410584.1').display | Changed value for display: 'Lead signal loss' vs 'leadsignal-loss'
Warning | CodeSystem.concept.where(code='8410584.2').display | Changed value for display: 'Lead wire loss first-lead' vs 'leadwire-loss-first-lead'
Warning | CodeSystem.concept.where(code='8410584.3').display | Changed value for display: 'Lead signal loss first-lead' vs 'leadsignal-loss-first-lead'
Warning | CodeSystem.concept.where(code='8410584.4').display | Changed value for display: 'Lead wire loss second-lead' vs 'leadwire-loss-second-lead'
Warning | CodeSystem.concept.where(code='8410584.5').display | Changed value for display: 'Lead signal loss second-lead' vs 'leadsignal-loss-second-lead'
Warning | CodeSystem.concept.where(code='8410584.6').display | Changed value for display: 'Lead wire loss third-lead' vs 'leadwire-loss-third-lead'
Warning | CodeSystem.concept.where(code='8410584.7').display | Changed value for display: 'Lead signal loss third-lead' vs 'leadsignal-loss-third-lead'
Warning | CodeSystem.concept.where(code='8417752.0').display | Changed value for display: 'Battery low' vs 'device-battery-low'
Warning | CodeSystem.concept.where(code='8417752.1').display | Changed value for display: 'Sensor malfunction' vs 'sensor-malfunction'
Warning | CodeSystem.concept.where(code='8417752.2').display | Changed value for display: 'Not enough blood in sample' vs 'sensor-sample-size-insufficient'
Warning | CodeSystem.concept.where(code='8417752.3').display | Changed value for display: 'Sensor strip insertion' vs 'sensor-strip-insertion'
Warning | CodeSystem.concept.where(code='8417752.4').display | Changed value for display: 'Sensor strip type incorrect' vs 'sensor-strip-type-incorrect'
Warning | CodeSystem.concept.where(code='8417752.5').display | Changed value for display: 'Sensor result too high' vs 'sensor-result-too-high'
Warning | CodeSystem.concept.where(code='8417752.6').display | Changed value for display: 'Sensor result too low' vs 'sensor-result-too-low'
Warning | CodeSystem.concept.where(code='8417752.7').display | Changed value for display: 'Sensor temp too high' vs 'sensor-temp-too-high'
Warning | CodeSystem.concept.where(code='8417752.8').display | Changed value for display: 'Sensor temp too low' vs 'sensor-temp-too-low'
Warning | CodeSystem.concept.where(code='8417752.9').display | Changed value for display: 'Sensor read interrupt' vs 'sensor-read-interrupt'
Warning | CodeSystem.concept.where(code='8417752.10').display | Changed value for display: 'General Device Fault' vs 'device-gen-fault'
Warning | CodeSystem.concept.where(code='8417752.11').display | Changed value for display: 'Sensor temp out of range' vs 'sensor-temp-out-of-range'
Warning | CodeSystem.concept.where(code='8417909.0').display | Changed value for display: 'INR device battery low' vs 'inr-device-battery-low'
Warning | CodeSystem.concept.where(code='8417909.1').display | Changed value for display: 'Sensor malfunction' vs 'inr-sensor-malfunction'
Warning | CodeSystem.concept.where(code='8417909.2').display | Changed value for display: 'Not enough blood in sample' vs 'inr-sensor-sample-size-insufficient'
Warning | CodeSystem.concept.where(code='8417909.3').display | Changed value for display: 'INR sensor strip insertion' vs 'inr-sensor-strip-insertion'
Warning | CodeSystem.concept.where(code='8417909.4').display | Changed value for display: 'INR sensor strip type incorrect' vs 'inr-sensor-strip-type-incorrect'
Warning | CodeSystem.concept.where(code='8417909.5').display | Changed value for display: 'INR sensor result too high' vs 'inr-sensor-result-too-high'
Warning | CodeSystem.concept.where(code='8417909.6').display | Changed value for display: 'INR sensor result too low' vs 'inr-sensor-result-too-low'
Warning | CodeSystem.concept.where(code='8417909.7').display | Changed value for display: 'INR sensor temp too high' vs 'inr-sensor-temp-too-high'
Warning | CodeSystem.concept.where(code='8417909.8').display | Changed value for display: 'INR sensor temp too low' vs 'inr-sensor-temp-too-low'
Warning | CodeSystem.concept.where(code='8417909.9').display | Changed value for display: 'INR sensor read interrupt' vs 'inr-sensor-read-interrupt'
Warning | CodeSystem.concept.where(code='8417909.10').display | Changed value for display: 'INR device general fault' vs 'inr-device-gen-fault'
Warning | CodeSystem.concept.where(code='8417909.11').display | Changed value for display: 'INR sensor calibration due' vs 'inr-sensor-calibration-due'
Warning | CodeSystem.concept.where(code='8408608.0').display | Changed value for display: 'Undetermined device status' vs 'device-status-undetermined'
Warning | CodeSystem.concept.where(code='8408608.1').display | Changed value for display: 'Device status reset' vs 'device-status-reset'
Warning | CodeSystem.concept.where(code='8408608.5').display | Changed value for display: 'Device status error' vs 'device-status-error'
Warning | CodeSystem.concept.where(code='8408608.6').display | Changed value for display: 'Device status error mechanical' vs 'device-status-error-mechanical'
Warning | CodeSystem.concept.where(code='8408608.7').display | Changed value for display: 'Device status error electronic' vs 'device-status-error-electronic'
Warning | CodeSystem.concept.where(code='8408608.8').display | Changed value for display: 'Device status error software' vs 'device-status-error-software'
Warning | CodeSystem.concept.where(code='8408608.9').display | Changed value for display: 'Device status error battery' vs 'device-status-error-battery'
Warning | CodeSystem.concept.where(code='8408608.15').display | Changed value for display: 'Device status service' vs 'device-status-service'
Information | CodeSystem.concept.where(code='8408608.15').definition | Changed value for definition: 'Undetermined device status event' vs 'Undetermined device status event, service needed'
Warning | CodeSystem.concept.where(code='8408608.16').display | Changed value for display: 'Device status service time-sync required' vs 'device-status-service-time-sync-required'
Warning | CodeSystem.concept.where(code='8408608.17').display | Changed value for display: 'Device status service calibration required' vs 'device-status-service-calibration-required'
Warning | CodeSystem.concept.where(code='8408608.18').display | Changed value for display: 'Device status service replentishment required' vs 'device-status-service-replenishment-required'
Information | CodeSystem.concept.where(code='8408608.18').definition | Changed value for definition: 'Replentishment required' vs 'Replenishment required'
Warning | CodeSystem.concept.where(code='8408608.25').display | Changed value for display: 'Device status battery low' vs 'device-status-battery-low'
Warning | CodeSystem.concept.where(code='8408608.26').display | Changed value for display: 'Device status battery depleted' vs 'device-status-battery-depleted'
Warning | CodeSystem.concept.where(code='8408608.27').display | Changed value for display: 'Device status battery replaced' vs 'device-status-battery-replaced'
Warning | CodeSystem.concept.where(code='8408608.28').display | Changed value for display: 'Device status battery interrupted' vs 'device-status-battery-interrupted'
Warning | CodeSystem.concept.where(code='8418060.0').display | Changed value for display: 'Sensor session stopped' vs 'sensor-session-stopped'
Warning | CodeSystem.concept.where(code='8418060.2').display | Changed value for display: 'Sensor type incorrect' vs 'sensor-type-incorrect'
Warning | CodeSystem.concept.where(code='8418060.3').display | Changed value for display: 'Sensor malfunction' vs 'sensor-malfunction'
Warning | CodeSystem.concept.where(code='8418060.4').display | Changed value for display: 'Device specific alert' vs 'device-specific-alert'
Warning | CodeSystem.concept.where(code='8418060.7').display | Changed value for display: 'Sensor calibration not allowed' vs 'sensor-calibration-not-allowed'
Warning | CodeSystem.concept.where(code='8418060.8').display | Changed value for display: 'Sensor calibration recommended' vs 'sensor-calibration-recommended'
Warning | CodeSystem.concept.where(code='8418060.9').display | Changed value for display: 'Sensor calibration required' vs 'sensor-calibration-required'
Warning | CodeSystem.concept.where(code='8418060.10').display | Changed value for display: 'Sensor temp too high' vs 'sensor-temp-too-high'
Warning | CodeSystem.concept.where(code='8418060.11').display | Changed value for display: 'Sensor temp too low' vs 'sensor-temp-too-low'
Warning | CodeSystem.concept.where(code='8418060.12').display | Changed value for display: 'Sensor result below patient level' vs 'sensor-result-below-patient-low'
Warning | CodeSystem.concept.where(code='8418060.13').display | Changed value for display: 'Sensor result above patient level' vs 'sensor-result-above-patient-high'
Warning | CodeSystem.concept.where(code='8418060.14').display | Changed value for display: 'Sensor low hypo' vs 'sensor-low-hypo'
Information | CodeSystem.concept.where(code='8418060.14').definition | Changed value for definition: 'Sensor result below the Hypo level' vs 'Sensor result below level'
Warning | CodeSystem.concept.where(code='8418060.15').display | Changed value for display: 'Sensor result hyper' vs 'sensor-high-hyper'
Information | CodeSystem.concept.where(code='8418060.15').definition | Changed value for definition: 'Sensor result above the Hyper level' vs 'Sensor result above level'
Warning | CodeSystem.concept.where(code='8418060.16').display | Changed value for display: 'Sensor rate decrease exceeded' vs 'sensor-rate-decrease-exceeded'
Warning | CodeSystem.concept.where(code='8418060.17').display | Changed value for display: 'Sensor rate increase exceeded' vs 'sensor-rate-increase-exceeded'
Warning | CodeSystem.concept.where(code='8418060.18').display | Changed value for display: 'Sensor result too low' vs 'sensor-result-too-low'
Warning | CodeSystem.concept.where(code='8418060.19').display | Changed value for display: 'Sensor result too high' vs 'sensor-result-too-high'
Warning | CodeSystem.concept.where(code='8418060.20').display | Changed value for display: 'Sensor com out of range' vs 'sensor-com-out-of-range'

### Metadata

Name | Value | Comments
--- | --- | ---
caseSensitive | true |
compositional |  |
content | complete |
copyright |  |
date | 2018-09-18T00:00:00+10:00 | 2018-09-18 | Values Differ
description | Maps IEEE 11073 ASN1 BITS measurements to codes. All these codes have two possible values, set or cleared. The code may either represent an event or a state. When an event, the defined event has occurred when set. If a state, the described item is either set or cleared. Sometimes the states may be defined in unexpected manners. For example, the regulation state when set is unregulated and when cleared it is regulated. In addition the code may derive from an IEEE 11073 attribute or from a measurement. More codes maybe added to this list in the future. |
experimental | true |
hierarchyMeaning |  | grouped-by | Added the item 'grouped-by'
jurisdiction |  |
jurisdiction[0] |  | http://unstats.un.org/unsd/methods/m49/m49.htm#001 | Added the item 'http://unstats.un.org/unsd/methods/m49/m49.htm#001'
name | ASN1ToHL7 |
publisher | Health Level Seven International (Health Care Devices Work Group) | HL7 International - Health Care Devices Work Group | Values Differ
purpose |  |
status | draft |
title |  |
url | http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7 |
version | 0.3.0 | 1.0.0 | Values Differ
versionNeeded |  |

### Concepts

Code | Display | type | source | Comments
--- | --- | --- | --- | ---
67925.0 | Mains power state | onMains | state | state | attribute | attribute | display changed from left to right
67925.1 | Battery state | onBattery | state | state | attribute | attribute | display changed from left to right
67925.8 | Charging at full rate | chargingFull | event | event | attribute | attribute | display changed from left to right
67925.9 | Charging at trickle rate | chargingTrickle | event | event | attribute | attribute | display changed from left to right
67925.10 | Charging state | chargingOff | state | state | attribute | attribute | display changed from left to right
532354.0 | If bit is cleared device is regulated | regulation-status | state | state | attribute | attribute | display changed from left to right definition changed from left to right
68219.0 | Real-time clock | mds-time-capab-real-time-clock | event | event | attribute | attribute | display changed from left to right
68219.1 | PHG set-time | mds-time-capab-set-clock | event | event | attribute | attribute | display changed from left to right
68219.2 | Relative Time | mds-time-capab-relative-time | event | event | attribute | attribute | display changed from left to right
68219.3 | Hi-Res Relative Time | mds-time-capab-high-res-relative-time | event | event | attribute | attribute | display changed from left to right
68219.4 | Sync Absolute Time | mds-time-capab-sync-abs-time | event | event | attribute | attribute | display changed from left to right
68219.5 | Sync Relative Time | mds-time-capab-sync-rel-time | event | event | attribute | attribute | display changed from left to right
68219.6 | Sync Hi-Res Relative Time | mds-time-capab-sync-hi-res-relative-time | event | event | attribute | attribute | display changed from left to right
68219.7 | Base Offset Time | mds-time-capab-bo-time | event | event | attribute | attribute | display changed from left to right
68219.8 | Absolute Time Synced | mds-time-state-abs-time-synced | event | event | attribute | attribute | display changed from left to right
68219.9 | Relative Time Synced | mds-time-state-rel-time-synced | event | event | attribute | attribute | display changed from left to right
68219.10 | Hi-Res Relative Time Synced | mds-time-state-hi-res-relative-time-synced | event | event | attribute | attribute | display changed from left to right
68219.11 | PHG Set-Time Requested | mds-time-mgr-set-time | event | event | attribute | attribute | display changed from left to right
68219.12 | Syncing base-offset time support | mds-time-capab-sync-bo-time | event | event | attribute | attribute | display changed from left to right
68219.13 | Base-Offset Time Synced | mds-time-state-bo-time-synced | event | event | attribute | attribute | display changed from left to right
68219.14 | Base-Offset Time UTC Aligned | mds-time-state-bo-time-UTC-aligned | event | event | attribute | attribute | display changed from left to right
68219.15 | Daylight Savings Time Rules Understood | mds-time-dst-rules-enabled | event | event | attribute | attribute | display changed from left to right
67846.0 | All alerts disabled | lim-alert-off | state | state | measurement | measurement | display changed from left to right
67846.1 | Low limit alert disabled | lim-low-off | state | state | measurement | measurement | display changed from left to right
67846.2 | High limit alert disabled | lim-high-off | state | state | measurement | measurement | display changed from left to right
150604.0 | Device not connected to sensor | sensor-disconnected | event | event | measurement | measurement | display changed from left to right
150604.1 | Sensor has malfunctioned | sensor-malfunction | event | event | measurement | measurement | display changed from left to right
150604.2 | Sensor incorrectly placed on user | sensor-displaced | event | event | measurement | measurement | display changed from left to right
150604.3 | Unsupported sensor | sensor-unsupported | event | event | measurement | measurement | display changed from left to right
150604.4 | Sensor off | sensor-off | event | event | measurement | measurement | display changed from left to right
150604.5 | Sensor interference | sensor-interference | event | event | measurement | measurement | display changed from left to right
150604.6 | Searching for signal | signal-searching | event | event | measurement | measurement | display changed from left to right
150604.7 | Signal pulse questionable | signal-pulse-questionable | event | event | measurement | measurement | display changed from left to right
150604.8 | Non pulsatile signal | signal-non-pulsatile | event | event | measurement | measurement | display changed from left to right
150604.9 | Signal erratic | signal-erratic | event | event | measurement | measurement | display changed from left to right
150604.10 | Signal low perfusion | signal-low-perfusion | event | event | measurement | measurement | display changed from left to right
150604.11 | Signal is poor | signal-poor | event | event | measurement | measurement | display changed from left to right
150604.12 | Signal inadequate | signal-inadequate | event | event | measurement | measurement | display changed from left to right
150604.13 | Signal experiencing processing irregularity | signal-processing-irregularity | event | event | measurement | measurement | display changed from left to right
150604.14 | Device malfunction | device-equipment-malfunction | event | event | measurement | measurement | display changed from left to right
150604.15 | Device extended update | device-extended-update | event | event | measurement | measurement | display changed from left to right
150605.0 | Pulse quality nominal | pulse-qual-nominal | event | event | measurement | measurement | display changed from left to right
150605.1 | Pulse quality marginal | pulse-qual-marginal | event | event | measurement | measurement | display changed from left to right
150605.2 | Pulse quality minimal | pulse-qual-minimal | event | event | measurement | measurement | display changed from left to right
150605.3 | Pulse quality unacceptable | pulse-qual-unacceptable | event | event | measurement | measurement | display changed from left to right
8410584.0 | Lead wire loss | leadwire-loss | event | event | measurement | measurement | display changed from left to right
8410584.1 | Lead signal loss | leadsignal-loss | event | event | measurement | measurement | display changed from left to right
8410584.2 | Lead wire loss first-lead | leadwire-loss-first-lead | event | event | measurement | measurement | display changed from left to right
8410584.3 | Lead signal loss first-lead | leadsignal-loss-first-lead | event | event | measurement | measurement | display changed from left to right
8410584.4 | Lead wire loss second-lead | leadwire-loss-second-lead | event | event | measurement | measurement | display changed from left to right
8410584.5 | Lead signal loss second-lead | leadsignal-loss-second-lead | event | event | measurement | measurement | display changed from left to right
8410584.6 | Lead wire loss third-lead | leadwire-loss-third-lead | event | event | measurement | measurement | display changed from left to right
8410584.7 | Lead signal loss third-lead | leadsignal-loss-third-lead | event | event | measurement | measurement | display changed from left to right
8417752.0 | Battery low | device-battery-low | event | event | measurement | measurement | display changed from left to right
8417752.1 | Sensor malfunction | sensor-malfunction | event | event | measurement | measurement | display changed from left to right
8417752.2 | Not enough blood in sample | sensor-sample-size-insufficient | event | event | measurement | measurement | display changed from left to right
8417752.3 | Sensor strip insertion | sensor-strip-insertion | event | event | measurement | measurement | display changed from left to right
8417752.4 | Sensor strip type incorrect | sensor-strip-type-incorrect | event | event | measurement | measurement | display changed from left to right
8417752.5 | Sensor result too high | sensor-result-too-high | event | event | measurement | measurement | display changed from left to right
8417752.6 | Sensor result too low | sensor-result-too-low | event | event | measurement | measurement | display changed from left to right
8417752.7 | Sensor temp too high | sensor-temp-too-high | event | event | measurement | measurement | display changed from left to right
8417752.8 | Sensor temp too low | sensor-temp-too-low | event | event | measurement | measurement | display changed from left to right
8417752.9 | Sensor read interrupt | sensor-read-interrupt | event | event | measurement | measurement | display changed from left to right
8417752.10 | General Device Fault | device-gen-fault | event | event | measurement | measurement | display changed from left to right
8417752.11 | Sensor temp out of range | sensor-temp-out-of-range | event | event | measurement | measurement | display changed from left to right
8417909.0 | INR device battery low | inr-device-battery-low | event | event | measurement | measurement | display changed from left to right
8417909.1 | Sensor malfunction | inr-sensor-malfunction | event | event | measurement | measurement | display changed from left to right
8417909.2 | Not enough blood in sample | inr-sensor-sample-size-insufficient | event | event | measurement | measurement | display changed from left to right
8417909.3 | INR sensor strip insertion | inr-sensor-strip-insertion | event | event | measurement | measurement | display changed from left to right
8417909.4 | INR sensor strip type incorrect | inr-sensor-strip-type-incorrect | event | event | measurement | measurement | display changed from left to right
8417909.5 | INR sensor result too high | inr-sensor-result-too-high | event | event | measurement | measurement | display changed from left to right
8417909.6 | INR sensor result too low | inr-sensor-result-too-low | event | event | measurement | measurement | display changed from left to right
8417909.7 | INR sensor temp too high | inr-sensor-temp-too-high | event | event | measurement | measurement | display changed from left to right
8417909.8 | INR sensor temp too low | inr-sensor-temp-too-low | event | event | measurement | measurement | display changed from left to right
8417909.9 | INR sensor read interrupt | inr-sensor-read-interrupt | event | event | measurement | measurement | display changed from left to right
8417909.10 | INR device general fault | inr-device-gen-fault | event | event | measurement | measurement | display changed from left to right
8417909.11 | INR sensor calibration due | inr-sensor-calibration-due | event | event | measurement | measurement | display changed from left to right
8408608.0 | Undetermined device status | device-status-undetermined | event | event | measurement | measurement | display changed from left to right
8408608.1 | Device status reset | device-status-reset | event | event | measurement | measurement | display changed from left to right
8408608.5 | Device status error | device-status-error | event | event | measurement | measurement | display changed from left to right
8408608.6 | Device status error mechanical | device-status-error-mechanical | event | event | measurement | measurement | display changed from left to right
8408608.7 | Device status error electronic | device-status-error-electronic | event | event | measurement | measurement | display changed from left to right
8408608.8 | Device status error software | device-status-error-software | event | event | measurement | measurement | display changed from left to right
8408608.9 | Device status error battery | device-status-error-battery | event | event | measurement | measurement | display changed from left to right
8408608.15 | Device status service | device-status-service | event | event | measurement | measurement | display changed from left to right definition changed from left to right
8408608.16 | Device status service time-sync required | device-status-service-time-sync-required | event | event | measurement | measurement | display changed from left to right
8408608.17 | Device status service calibration required | device-status-service-calibration-required | event | event | measurement | measurement | display changed from left to right
8408608.18 | Device status service replentishment required | device-status-service-replenishment-required | event | event | measurement | measurement | display changed from left to right definition changed from left to right
8408608.25 | Device status battery low | device-status-battery-low | event | event | measurement | measurement | display changed from left to right
8408608.26 | Device status battery depleted | device-status-battery-depleted | event | event | measurement | measurement | display changed from left to right
8408608.27 | Device status battery replaced | device-status-battery-replaced | event | event | measurement | measurement | display changed from left to right
8408608.28 | Device status battery interrupted | device-status-battery-interrupted | event | event | measurement | measurement | display changed from left to right
8418060.0 | Sensor session stopped | sensor-session-stopped | event | event | measurement | measurement | display changed from left to right
8418060.2 | Sensor type incorrect | sensor-type-incorrect | event | event | measurement | measurement | display changed from left to right
8418060.3 | Sensor malfunction | sensor-malfunction | event | event | measurement | measurement | display changed from left to right
8418060.4 | Device specific alert | device-specific-alert | event | event | measurement | measurement | display changed from left to right
8418060.7 | Sensor calibration not allowed | sensor-calibration-not-allowed | event | event | measurement | measurement | display changed from left to right
8418060.8 | Sensor calibration recommended | sensor-calibration-recommended | event | event | measurement | measurement | display changed from left to right
8418060.9 | Sensor calibration required | sensor-calibration-required | event | event | measurement | measurement | display changed from left to right
8418060.10 | Sensor temp too high | sensor-temp-too-high | event | event | measurement | measurement | display changed from left to right
8418060.11 | Sensor temp too low | sensor-temp-too-low | event | event | measurement | measurement | display changed from left to right
8418060.12 | Sensor result below patient level | sensor-result-below-patient-low | event | event | measurement | measurement | display changed from left to right
8418060.13 | Sensor result above patient level | sensor-result-above-patient-high | event | event | measurement | measurement | display changed from left to right
8418060.14 | Sensor low hypo | sensor-low-hypo | event | event | measurement | measurement | display changed from left to right definition changed from left to right
8418060.15 | Sensor result hyper | sensor-high-hyper | event | event | measurement | measurement | display changed from left to right definition changed from left to right
8418060.16 | Sensor rate decrease exceeded | sensor-rate-decrease-exceeded | event | event | measurement | measurement | display changed from left to right
8418060.17 | Sensor rate increase exceeded | sensor-rate-increase-exceeded | event | event | measurement | measurement | display changed from left to right
8418060.18 | Sensor result too low | sensor-result-too-low | event | event | measurement | measurement | display changed from left to right
8418060.19 | Sensor result too high | sensor-result-too-high | event | event | measurement | measurement | display changed from left to right
8418060.20 | Sensor com out of range | sensor-com-out-of-range | event | event | measurement | measurement | display changed from left to right
8418512.0 |  | Battery-status-Undetermined |  |  |  |  | Added this concept
8418512.1 |  | Battery-absent |  |  |  |  | Added this concept
8418512.2 |  | Battery-active |  |  |  |  | Added this concept
8418512.3 |  | Battery-charging |  |  |  |  | Added this concept
8418512.4 |  | Battery-fullyCharged |  |  |  |  | Added this concept
8418512.5 |  | Battery-disposable |  |  |  |  | Added this concept
8418512.6 |  | Battery-rechargeable |  |  |  |  | Added this concept
8418512.8 |  | Battery-faulty |  |  |  |  | Added this concept
8418512.9 |  | Battery-incompatible |  |  |  |  | Added this concept
8410608.0 |  | body-movement |  |  |  |  | Added this concept
8410608.1 |  | cuff-too-loose |  |  |  |  | Added this concept
8410608.2 |  | irregular-pulse |  |  |  |  | Added this concept
8410608.3 |  | pulse-over-range-limit |  |  |  |  | Added this concept
8410608.4 |  | pulse-under-range-limit |  |  |  |  | Added this concept
8410608.5 |  | improper-body-position |  |  |  |  | Added this concept