Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## CodeSystem: Measurement status codes

Summary

Defining URL: | http://hl7.org/fhir/uv/pocd/CodeSystem/measurement-status
Version: | 1.0.0
Name: | MeasurementStatus
Title: | Measurement status codes
Status: | Draft as of 2019-09-28
Definition: | Measurement status definitions from the ISO/IEEE 11073-10201 DIM.
Publisher: | HL7 International - Health Care Devices Work Group
Content: | Complete: All the concepts defined by the code system are included in the code system resource
Source Resource: | XML / JSON / Turtle

This Code system is referenced in the content logical definition of the following value sets:

This CodeSystem is not used here; it may be used elsewhere (e.g. specifications and/or implementations that use this content)

This code system http://hl7.org/fhir/uv/pocd/CodeSystem/measurement-status defines the following codes:

Code | Display | Definition
questionable | Questionable | Data may not be reliable
calibration-ongoing | Calibration ongoing | Calibration is ongoing
validated-data | Validated data | Relevant, e.g., in an archive
early-indication | Early indication | Early estimate of value
msmt-ongoing | Measurement ongoing | Indicates that a new measurement is just being taken
in-alarm | Measurement in alarm | Measurement has an active alarm condition
alarm-inhibited | Measurement alarms inhibited | Measurement supports alarming and alarms are turned off