Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## Example Device: Example of a Gateway

Generated Narrative

Resource "phg-ecde3d4e58532d31.000000000000"

Profile: PhgDevice

identifier: IEEE 11073 System Identifier: ec-de-3d-4e-58-53-2d-31, Bluetooth MAC address: 3d-4e-58-53-2d-31, Ethernet MAC address: 3d-4e-58-53-2d-35

type: MDC_MOC_VMS_MDS_AHD (ISO 11073-10101 Health informatics - Point-of-care#531981)

### Versions

- | Type | Value
* | MDC_REG_CERT_DATA_CONTINUA_VERSION: Continua version (ISO 11073-10101 Health informatics - Point-of-care#532352) | 5.0

> property

> type: MDC_TIME_SYNC_PROTOCOL: Time synchronization protocol (ISO 11073-10101 Health informatics - Point-of-care#68220)

> valueCode: MDC_TIME_SYNC_NTPV4: (ISO 11073-10101 Health informatics - Point-of-care#532226)

> property

> type: MDC_REG_CERT_DATA_CONTINUA_CERT_DEV_LIST: certified device list as transport-specialization combo (ISO 11073-10101 Health informatics - Point-of-care#532353)

> valueCode: Pulse Oximeter certified (ContinuaPHD#4)

> property

> type: MDC_REG_CERT_DATA_CONTINUA_AHD_CERT_LIST: certified Upload classes (ISO 11073-10101 Health informatics - Point-of-care#532355)

> valueCode: observation-upload-soap (ContinuaHFS#0), observation-upload-hdata (ContinuaHFS#3), observation-upload-fhir (ContinuaHFS#7), capabilities (ContinuaHFS#2), aps (ContinuaHFS#6)

> property

> type: regulation-status (ASN1ToHL7#532354.0)

> valueCode: Device is not regulated (v2 Y/N Indicator#Y)