Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## : Measurement status codes - JSON Representation

Raw json | Download

    {
      "resourceType" : "CodeSystem",
      "id" : "measurement-status",
      "meta" : {
        "profile" : [
          "http://hl7.org/fhir/StructureDefinition/shareablecodesystem"
        ]
      },
      "text" : {
        "status" : "generated",
        "div" : "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p>This code system http://hl7.org/fhir/uv/pocd/CodeSystem/measurement-status defines the following codes:</p><table class=\"codes\"><tr><td style=\"white-space:nowrap\"><b>Code</b></td><td><b>Display</b></td><td><b>Definition</b></td></tr><tr><td style=\"white-space:nowrap\">questionable<a name=\"measurement-status-questionable\"> </a></td><td>Questionable</td><td>Data may not be reliable</td></tr><tr><td style=\"white-space:nowrap\">calibration-ongoing<a name=\"measurement-status-calibration-ongoing\"> </a></td><td>Calibration ongoing</td><td>Calibration is ongoing</td></tr><tr><td style=\"white-space:nowrap\">validated-data<a name=\"measurement-status-validated-data\"> </a></td><td>Validated data</td><td>Relevant, e.g., in an archive</td></tr><tr><td style=\"white-space:nowrap\">early-indication<a name=\"measurement-status-early-indication\"> </a></td><td>Early indication</td><td>Early estimate of value</td></tr><tr><td style=\"white-space:nowrap\">msmt-ongoing<a name=\"measurement-status-msmt-ongoing\"> </a></td><td>Measurement ongoing</td><td>Indicates that a new measurement is just being taken</td></tr><tr><td style=\"white-space:nowrap\">in-alarm<a name=\"measurement-status-in-alarm\"> </a></td><td>Measurement in alarm</td><td>Measurement has an active alarm condition</td></tr><tr><td style=\"white-space:nowrap\">alarm-inhibited<a name=\"measurement-status-alarm-inhibited\"> </a></td><td>Measurement alarms inhibited</td><td>Measurement supports alarming and alarms are turned off</td></tr></table></div>"
      },
      "url" : "http://hl7.org/fhir/uv/pocd/CodeSystem/measurement-status",
      "version" : "1.0.0",
      "name" : "MeasurementStatus",
      "title" : "Measurement status codes",
      "status" : "draft",
      "experimental" : false,
      "date" : "2019-09-28",
      "publisher" : "HL7 International - Health Care Devices Work Group",
      "contact" : [
        {
          "telecom" : [
            {
              "system" : "url",
              "value" : "http://hl7.org/Special/committees/healthcaredevices"
            }
          ]
        }
      ],
      "description" : "Measurement status definitions from the ISO/IEEE 11073-10201 DIM.",
      "jurisdiction" : [
        {
          "coding" : [
            {
              "system" : "http://unstats.un.org/unsd/methods/m49/m49.htm",
              "code" : "001"
            }
          ]
        }
      ],
      "caseSensitive" : false,
      "hierarchyMeaning" : "grouped-by",
      "content" : "complete",
      "concept" : [
        {
          "code" : "questionable",
          "display" : "Questionable",
          "definition" : "Data may not be reliable"
        },
        {
          "code" : "calibration-ongoing",
          "display" : "Calibration ongoing",
          "definition" : "Calibration is ongoing"
        },
        {
          "code" : "validated-data",
          "display" : "Validated data",
          "definition" : "Relevant, e.g., in an archive"
        },
        {
          "code" : "early-indication",
          "display" : "Early indication",
          "definition" : "Early estimate of value"
        },
        {
          "code" : "msmt-ongoing",
          "display" : "Measurement ongoing",
          "definition" : "Indicates that a new measurement is just being taken"
        },
        {
          "code" : "in-alarm",
          "display" : "Measurement in alarm",
          "definition" : "Measurement has an active alarm condition"
        },
        {
          "code" : "alarm-inhibited",
          "display" : "Measurement alarms inhibited",
          "definition" : "Measurement supports alarming and alarms are turned off"
        }
      ]
    }