Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## Example Device: Example of PHD Device

Generated Narrative

Resource "phd-74E8FFFEFF051C00.001C05FFE874"

Profile: PhdDevice

identifier: IEEE 11073 System Identifier: 74-E8-FF-FE-FF-05-1C-00, Bluetooth MAC address: 00-1C-05-FF-E8-74

manufacturer: Nonin_Medical_Inc.

serialNumber: 501900083

modelNumber: Model 3230

type: MDC_MOC_VMS_MDS_SIMP (ISO 11073-10101 Health informatics - Point-of-care#65573)

### Specializations

- | SystemType | Version
* | MDC_DEV_SPEC_PROFILE_PULS_OXIM: Pulse Oximeter (ISO 11073-10101 Health informatics - Point-of-care#528388) | 1

> version

> type: MDC_ID_PROD_SPEC_FW: Firmware revision (ISO 11073-10101 Health informatics - Point-of-care#531976)

> value: r2.1

> version

> type: MDC_ID_PROD_SPEC_SW: Software revision (ISO 11073-10101 Health informatics - Point-of-care#531975)

> value: r1.5 9.7

> version

> type: MDC_ID_PROD_SPEC_HW: Hardware revision (ISO 11073-10101 Health informatics - Point-of-care#531974)

> value: r1.0

> version

> type: MDC_REG_CERT_DATA_CONTINUA_VERSION: Continua version (ISO 11073-10101 Health informatics - Point-of-care#532352)

> value: 6.0

> property

> type: MDC_REG_CERT_DATA_CONTINUA_CERT_DEV_LIST: certified device list as transport-specialization combo (ISO 11073-10101 Health informatics - Point-of-care#532353)

> valueCode: BTLE Pulse Oximeter certified (ContinuaPHD#32772)

> property

> type: regulation-status (ASN1ToHL7#532354.0)

> valueCode: Device is Regulated (v2 Y/N Indicator#N)

> property

> type: MDC_TIME_SYNC_PROTOCOL: Time synchronization protocol (ISO 11073-10101 Health informatics - Point-of-care#68220)

> valueCode: MDC_TIME_SYNC_NONE: (ISO 11073-10101 Health informatics - Point-of-care#532224)