Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## ValueSet: ASN1attribute

Summary

Defining URL: | http://hl7.org/fhir/uv/phd/ValueSet/ASN1attribute
Version: | 1.0.0
Name: | ASN1attribute
Title: | ANS1ToHL7 codes defined for non-measurement attributes
Status: | Draft as of 2018-09-17
Definition: | ValueSet for the ANS1ToHL7 codes that are not derived from enumeration measurements.
Publisher: | HL7 International - Health Care Devices Work Group
Source Resource: | XML / JSON / Turtle

References

- PhdDevice
- PhdNumericObservation
- PhgDevice

### Logical Definition (CLD)

- Include codes from `http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7` where source = attribute

### Expansion

This value set contains 22 concepts

Expansion based on ASN1ToHL7 v1.0.0 (CodeSystem)

All codes in this table are from the system `http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7`

Code | Display | Definition
67925.0 | onMains | Indicates whether the PHD is on or off mains power
67925.1 | onBattery | Indicates whether the PHD is on or off Battery power
67925.8 | chargingFull | Indicates whether the PHD battery is charging at maximum rate
67925.9 | chargingTrickle | Indicates whether the PHD battery is charging at a trickle rate
67925.10 | chargingOff | Indicates whether the PHD battery charging is on or off
532354.0 | regulation-status | Indicates device is regulated when cleared
68219.0 | mds-time-capab-real-time-clock | Indicates real time clock is supported
68219.1 | mds-time-capab-set-clock | Indicates support for the PHG to set the time
68219.2 | mds-time-capab-relative-time | Indicates Relative Time is supported
68219.3 | mds-time-capab-high-res-relative-time | Indicates Hi-Res Relative Time is supported
68219.4 | mds-time-capab-sync-abs-time | Indicates that syncing the absolute time is supported
68219.5 | mds-time-capab-sync-rel-time | Indicates that syncing the relative time is supported
68219.6 | mds-time-capab-sync-hi-res-relative-time | Indicates that syncing hi-res relative time is supported
68219.7 | mds-time-capab-bo-time | Indicates that the real-time clock supports base offset time
68219.8 | mds-time-state-abs-time-synced | Indicates the absolute time has been synced
68219.9 | mds-time-state-rel-time-synced | Indicates the relative time has been synced
68219.10 | mds-time-state-hi-res-relative-time-synced | Indicates the hi-res time has been synced
68219.11 | mds-time-mgr-set-time | PHG Requested to set the time
68219.12 | mds-time-capab-sync-bo-time | Indicates that syncing base-offset time is supported
68219.13 | mds-time-state-bo-time-synced | Indicates that base-offset time has been synced
68219.14 | mds-time-state-bo-time-UTC-aligned | Indicates that base-offset time is aligned with UTC time standard
68219.15 | mds-time-dst-rules-enabled | Indicates support for daylight savings time rules

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
Source | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code