Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## ValueSet: ASN1measurement

Summary

Defining URL: | http://hl7.org/fhir/uv/phd/ValueSet/ASN1measurement
Version: | 1.0.0
Name: | ASN1measurement
Title: | ANS1ToHL7 codes defined for measurement attributes
Status: | Draft as of 2018-09-17
Definition: | ValueSet for the ANS1ToHL7 codes that are derived from enumeration measurements.
Publisher: | HL7 International - Health Care Devices Work Group
Source Resource: | XML / JSON / Turtle

References

- PhdBitsEnumerationObservation

### Logical Definition (CLD)

- Include codes from `http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7` where source = measurement

### Expansion

This value set contains 104 concepts

Expansion based on ASN1ToHL7 v1.0.0 (CodeSystem)

All codes in this table are from the system `http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7`

Level | Code | Display | Definition
1 | 67846.0 | lim-alert-off | Indicates both the high and the low limit alerts are disabled
1 | 67846.1 | lim-low-off | Indicates the low limit alert is disabled
1 | 67846.2 | lim-high-off | Indicates the high limit alert is disabled
1 | 150604.0 | sensor-disconnected | Indicates the device is not connected with the sensor
1 | 150604.1 | sensor-malfunction | Indicates the sensor has malfunctioned
1 | 150604.2 | sensor-displaced | Indicates the sensor is not correctly placed on the user
1 | 150604.3 | sensor-unsupported | Indicates the sensor connected to the device is unsupported
1 | 150604.4 | sensor-off | Indicates the sensor is not connected to the user
1 | 150604.5 | sensor-interference | Indicates the sensor is experiencing interference
1 | 150604.6 | signal-searching | Indicates the sensor is searching for a signal
1 | 150604.7 | signal-pulse-questionable | Indicates a questionable pulse has been detected
1 | 150604.8 | signal-non-pulsatile | Indicates a non pulsatile signal has been detected
1 | 150604.9 | signal-erratic | Indicates a signal has been discovered, but it is erratic
1 | 150604.10 | signal-low-perfusion | Indicates the signal is experiencing low perfusion
1 | 150604.11 | signal-poor | Indicates the signal has been discovered, but it is poor
1 | 150604.12 | signal-inadequate | Indicates the signal has been discovered, but it is inadequate
1 | 150604.13 | signal-processing-irregularity | Indicates the signal has been discovered, but is experiencing processing irregularity
1 | 150604.14 | device-equipment-malfunction | Indicates a device malfunction has occurred
1 | 150604.15 | device-extended-update | Indicates an extended display update is in progress on device
1 | 150605.0 | pulse-qual-nominal | Indicates no abnormalities have been detected by the sensor
1 | 150605.1 | pulse-qual-marginal | Indicates the pulse profusion or quality is marginal
1 | 150605.2 | pulse-qual-minimal | Indicates the pulse profusion or quality is minimal
1 | 150605.3 | pulse-qual-unacceptable | Indicates the pulse profusion or quality is unacceptable
1 | 8410584.0 | leadwire-loss | Loss of unspecified lead wire or electrode connection
1 | 8410584.1 | leadsignal-loss | Loss of unspecified lead signal
1 | 8410584.2 | leadwire-loss-first-lead | Loss of 1st lead wire or electrode connection
1 | 8410584.3 | leadsignal-loss-first-lead | Loss of 1st lead signal
1 | 8410584.4 | leadwire-loss-second-lead | Loss of 2nd lead wire or electrode connection
1 | 8410584.5 | leadsignal-loss-second-lead | Loss of 2nd lead signal
1 | 8410584.6 | leadwire-loss-third-lead | Loss of 3rd lead wire or electrode connection
1 | 8410584.7 | leadsignal-loss-third-lead | Loss of 3rd lead signal
1 | 8417752.0 | device-battery-low | The device battery is low
1 | 8417752.1 | sensor-malfunction | The sensor has malfunctioned
1 | 8417752.2 | sensor-sample-size-insufficient | The sensor's sample size is insufficient
1 | 8417752.3 | sensor-strip-insertion | The test strip was inserted incorrectly
1 | 8417752.4 | sensor-strip-type-incorrect | The test strip type is incompatable with the sensor
1 | 8417752.5 | sensor-result-too-high | The value reported by the sensor is too high
1 | 8417752.6 | sensor-result-too-low | The value reported by the sensor is too low
1 | 8417752.7 | sensor-temp-too-high | The temperature is too high
1 | 8417752.8 | sensor-temp-too-low | The temperature is too low
1 | 8417752.9 | sensor-read-interrupt | The read process was interrupted
1 | 8417752.10 | device-gen-fault | General Device Fault
1 | 8417752.11 | sensor-temp-out-of-range | The temperature is out of range
1 | 8417909.0 | inr-device-battery-low | The INR device battery is low
1 | 8417909.1 | inr-sensor-malfunction | The INR device sensor has malfunctioned
1 | 8417909.2 | inr-sensor-sample-size-insufficient | The sample size was insufficient
1 | 8417909.3 | inr-sensor-strip-insertion | The test script was inserted incorrectly
1 | 8417909.4 | inr-sensor-strip-type-incorrect | The test strip used is not compatible with the INR
1 | 8417909.5 | inr-sensor-result-too-high | The test result is too high
1 | 8417909.6 | inr-sensor-result-too-low | The test result is too low
1 | 8417909.7 | inr-sensor-temp-too-high | The temperature is too high
1 | 8417909.8 | inr-sensor-temp-too-low | The temperature is too low
1 | 8417909.9 | inr-sensor-read-interrupt | The read process was interrupted
1 | 8417909.10 | inr-device-gen-fault | General device fault
1 | 8417909.11 | inr-sensor-calibration-due | The INR sensor calibration is due
1 | 8408608.0 | device-status-undetermined | Undetermined device status event
1 | 8408608.1 | device-status-reset | Device reset
1 | 8408608.5 | device-status-error | Device error
1 | 8408608.6 | device-status-error-mechanical | Mechanical error
1 | 8408608.7 | device-status-error-electronic | Electronic error
1 | 8408608.8 | device-status-error-software | Software error
1 | 8408608.9 | device-status-error-battery | Battery error
1 | 8408608.15 | device-status-service | Undetermined device status event, service needed
1 | 8408608.16 | device-status-service-time-sync-required | Time sync service required
1 | 8408608.17 | device-status-service-calibration-required | Calibration required
1 | 8408608.18 | device-status-service-replenishment-required | Replenishment required
1 | 8408608.25 | device-status-battery-low | Battery power is too low
1 | 8408608.26 | device-status-battery-depleted | Battery is depleted
1 | 8408608.27 | device-status-battery-replaced | Battery has been replaced
1 | 8408608.28 | device-status-battery-interrupted | Battery was interrupted
1 | 8418060.0 | sensor-session-stopped | Session stopped
1 | 8418060.2 | sensor-type-incorrect | Sensor type incorrect for device
1 | 8418060.3 | sensor-malfunction | The sensor malfunctioned
1 | 8418060.4 | device-specific-alert | Device specific alert
1 | 8418060.7 | sensor-calibration-not-allowed | Calibrating the sensor is not allowed
1 | 8418060.8 | sensor-calibration-recommended | Calibrating the sensor is recommended
1 | 8418060.9 | sensor-calibration-required | Calibrating the sensor is required
1 | 8418060.10 | sensor-temp-too-high | Temperature is too high for a valid result
1 | 8418060.11 | sensor-temp-too-low | Temperature is too low for a valid result
1 | 8418060.12 | sensor-result-below-patient-low | Sensor result below the Patient Low level
1 | 8418060.13 | sensor-result-above-patient-high | Sensor result above the Patient High level
1 | 8418060.14 | sensor-low-hypo | Sensor result below level
1 | 8418060.15 | sensor-high-hyper | Sensor result above level
1 | 8418060.16 | sensor-rate-decrease-exceeded | The sensor rate of decrease has been exceeded
1 | 8418060.17 | sensor-rate-increase-exceeded | The sensor rate of increase has been exceeded
1 | 8418060.18 | sensor-result-too-low | Sensor result is lower than the device can process
1 | 8418060.19 | sensor-result-too-high | Sensor result is higher than the device can process
1 | 8418060.20 | sensor-com-out-of-range | The sensor communication is out of range
1 | 8418512.0 | Battery-status-Undetermined | the status of the battery is unknown
1 | 8418512.1 | Battery-absent | Indicates if the battery is absent
1 | 8418512.2 | Battery-active | Indicates if the battery is active in the system
1 | 8418512.3 | Battery-charging | Indicates if the battery is charging
1 | 8418512.4 | Battery-fullyCharged | Indicates if the battery is fully charged
1 | 8418512.5 | Battery-disposable | Indicates if the battery is disposable
1 | 8418512.6 | Battery-rechargeable | Indicates if battery is rechargable
1 | 8418512.8 | Battery-faulty | Indicates if battery is faulty
2 | 8418512.7 | Battery-overTemperature | Indicates if the battery is too hot
1 | 8418512.9 | Battery-incompatible | Indicates if battery is incompatible
1 | 8410608.0 | body-movement | Indicates too much body movement
1 | 8410608.1 | cuff-too-loose | Indicates the cuff was too loose
1 | 8410608.2 | irregular-pulse | Indicates an irregular pulse was detected
1 | 8410608.3 | pulse-over-range-limit | Indicates the pulse was too high for sensor to work
1 | 8410608.4 | pulse-under-range-limit | Indicates the pulse was too low for sensor to work
1 | 8410608.5 | improper-body-position | Indicates the cuff was incorrectly placed with respect to the heart

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
Source | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code