## ValueSet Comparison between http://hl7.org/fhir/uv/phd/ValueSet/ASN1measurement vs http://hl7.org/fhir/uv/phd/ValueSet/ASN1measurement

### Messages

Error | ValueSet.version | Values for version differ: '0.3.0' vs '1.0.0'
Information | ValueSet.date | Values for date differ: '2018-09-17T00:00:00+10:00' vs '2018-09-17'
Information | ValueSet.publisher | Values for publisher differ: 'Health Level Seven International (Health Care Devices Work Group)' vs 'HL7 International - Health Care Devices Work Group'
Information | ValueSet.jurisdiction | Added the item 'http://unstats.un.org/unsd/methods/m49/m49.htm#001'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'All alerts disabled' vs 'lim-alert-off'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Low limit alert disabled' vs 'lim-low-off'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'High limit alert disabled' vs 'lim-high-off'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device not connected to sensor' vs 'sensor-disconnected'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor has malfunctioned' vs 'sensor-malfunction'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor incorrectly placed on user' vs 'sensor-displaced'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Unsupported sensor' vs 'sensor-unsupported'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor off' vs 'sensor-off'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor interference' vs 'sensor-interference'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Searching for signal' vs 'signal-searching'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Signal pulse questionable' vs 'signal-pulse-questionable'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Non pulsatile signal' vs 'signal-non-pulsatile'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Signal erratic' vs 'signal-erratic'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Signal low perfusion' vs 'signal-low-perfusion'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Signal is poor' vs 'signal-poor'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Signal inadequate' vs 'signal-inadequate'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Signal experiencing processing irregularity' vs 'signal-processing-irregularity'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device malfunction' vs 'device-equipment-malfunction'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device extended update' vs 'device-extended-update'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Pulse quality nominal' vs 'pulse-qual-nominal'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Pulse quality marginal' vs 'pulse-qual-marginal'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Pulse quality minimal' vs 'pulse-qual-minimal'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Pulse quality unacceptable' vs 'pulse-qual-unacceptable'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Lead wire loss' vs 'leadwire-loss'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Lead signal loss' vs 'leadsignal-loss'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Lead wire loss first-lead' vs 'leadwire-loss-first-lead'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Lead signal loss first-lead' vs 'leadsignal-loss-first-lead'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Lead wire loss second-lead' vs 'leadwire-loss-second-lead'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Lead signal loss second-lead' vs 'leadsignal-loss-second-lead'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Lead wire loss third-lead' vs 'leadwire-loss-third-lead'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Lead signal loss third-lead' vs 'leadsignal-loss-third-lead'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Battery low' vs 'device-battery-low'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor malfunction' vs 'sensor-malfunction'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Not enough blood in sample' vs 'sensor-sample-size-insufficient'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor strip insertion' vs 'sensor-strip-insertion'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor strip type incorrect' vs 'sensor-strip-type-incorrect'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor result too high' vs 'sensor-result-too-high'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor result too low' vs 'sensor-result-too-low'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor temp too high' vs 'sensor-temp-too-high'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor temp too low' vs 'sensor-temp-too-low'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor read interrupt' vs 'sensor-read-interrupt'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'General Device Fault' vs 'device-gen-fault'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor temp out of range' vs 'sensor-temp-out-of-range'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'INR device battery low' vs 'inr-device-battery-low'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor malfunction' vs 'inr-sensor-malfunction'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Not enough blood in sample' vs 'inr-sensor-sample-size-insufficient'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'INR sensor strip insertion' vs 'inr-sensor-strip-insertion'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'INR sensor strip type incorrect' vs 'inr-sensor-strip-type-incorrect'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'INR sensor result too high' vs 'inr-sensor-result-too-high'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'INR sensor result too low' vs 'inr-sensor-result-too-low'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'INR sensor temp too high' vs 'inr-sensor-temp-too-high'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'INR sensor temp too low' vs 'inr-sensor-temp-too-low'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'INR sensor read interrupt' vs 'inr-sensor-read-interrupt'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'INR device general fault' vs 'inr-device-gen-fault'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'INR sensor calibration due' vs 'inr-sensor-calibration-due'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Undetermined device status' vs 'device-status-undetermined'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status reset' vs 'device-status-reset'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status error' vs 'device-status-error'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status error mechanical' vs 'device-status-error-mechanical'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status error electronic' vs 'device-status-error-electronic'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status error software' vs 'device-status-error-software'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status error battery' vs 'device-status-error-battery'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status service' vs 'device-status-service'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status service time-sync required' vs 'device-status-service-time-sync-required'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status service calibration required' vs 'device-status-service-calibration-required'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status service replentishment required' vs 'device-status-service-replenishment-required'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status battery low' vs 'device-status-battery-low'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status battery depleted' vs 'device-status-battery-depleted'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status battery replaced' vs 'device-status-battery-replaced'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device status battery interrupted' vs 'device-status-battery-interrupted'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor session stopped' vs 'sensor-session-stopped'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor type incorrect' vs 'sensor-type-incorrect'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor malfunction' vs 'sensor-malfunction'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Device specific alert' vs 'device-specific-alert'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor calibration not allowed' vs 'sensor-calibration-not-allowed'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor calibration recommended' vs 'sensor-calibration-recommended'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor calibration required' vs 'sensor-calibration-required'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor temp too high' vs 'sensor-temp-too-high'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor temp too low' vs 'sensor-temp-too-low'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor result below patient level' vs 'sensor-result-below-patient-low'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor result above patient level' vs 'sensor-result-above-patient-high'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor low hypo' vs 'sensor-low-hypo'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor result hyper' vs 'sensor-high-hyper'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor rate decrease exceeded' vs 'sensor-rate-decrease-exceeded'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor rate increase exceeded' vs 'sensor-rate-increase-exceeded'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor result too low' vs 'sensor-result-too-low'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor result too high' vs 'sensor-result-too-high'
Warning | ValueSet.expansion.contains.name | Changed value for display: 'Sensor com out of range' vs 'sensor-com-out-of-range'

### Metadata

Name | Value | Comments
--- | --- | ---
compose.inactive |  |
compose.lockedDate |  |
copyright |  |
date | 2018-09-17T00:00:00+10:00 | 2018-09-17 | Values Differ
description | ValueSet for the ANS1ToHL7 codes that are derived from enumeration measurements. |
experimental | false |
immutable |  |
jurisdiction |  |
jurisdiction[0] |  | http://unstats.un.org/unsd/methods/m49/m49.htm#001 | Added the item 'http://unstats.un.org/unsd/methods/m49/m49.htm#001'
name | ASN1measurement |
publisher | Health Level Seven International (Health Care Devices Work Group) | HL7 International - Health Care Devices Work Group | Values Differ
purpose |  |
status | draft |
title | ANS1ToHL7 codes defined for measurement attributes |
url | http://hl7.org/fhir/uv/phd/ValueSet/ASN1measurement |
version | 0.3.0 | 1.0.0 | Values Differ

### Definition

Item | Property | Value | Comments
--- | --- | --- | ---
include | http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7 |  |

### Expansion

Code | Display | Comments
--- | --- | ---
67846.0 | All alerts disabled | lim-alert-off | display changed from left to right
67846.1 | Low limit alert disabled | lim-low-off | display changed from left to right
67846.2 | High limit alert disabled | lim-high-off | display changed from left to right
150604.0 | Device not connected to sensor | sensor-disconnected | display changed from left to right
150604.1 | Sensor has malfunctioned | sensor-malfunction | display changed from left to right
150604.2 | Sensor incorrectly placed on user | sensor-displaced | display changed from left to right
150604.3 | Unsupported sensor | sensor-unsupported | display changed from left to right
150604.4 | Sensor off | sensor-off | display changed from left to right
150604.5 | Sensor interference | sensor-interference | display changed from left to right
150604.6 | Searching for signal | signal-searching | display changed from left to right
150604.7 | Signal pulse questionable | signal-pulse-questionable | display changed from left to right
150604.8 | Non pulsatile signal | signal-non-pulsatile | display changed from left to right
150604.9 | Signal erratic | signal-erratic | display changed from left to right
150604.10 | Signal low perfusion | signal-low-perfusion | display changed from left to right
150604.11 | Signal is poor | signal-poor | display changed from left to right
150604.12 | Signal inadequate | signal-inadequate | display changed from left to right
150604.13 | Signal experiencing processing irregularity | signal-processing-irregularity | display changed from left to right
150604.14 | Device malfunction | device-equipment-malfunction | display changed from left to right
150604.15 | Device extended update | device-extended-update | display changed from left to right
150605.0 | Pulse quality nominal | pulse-qual-nominal | display changed from left to right
150605.1 | Pulse quality marginal | pulse-qual-marginal | display changed from left to right
150605.2 | Pulse quality minimal | pulse-qual-minimal | display changed from left to right
150605.3 | Pulse quality unacceptable | pulse-qual-unacceptable | display changed from left to right
8410584.0 | Lead wire loss | leadwire-loss | display changed from left to right
8410584.1 | Lead signal loss | leadsignal-loss | display changed from left to right
8410584.2 | Lead wire loss first-lead | leadwire-loss-first-lead | display changed from left to right
8410584.3 | Lead signal loss first-lead | leadsignal-loss-first-lead | display changed from left to right
8410584.4 | Lead wire loss second-lead | leadwire-loss-second-lead | display changed from left to right
8410584.5 | Lead signal loss second-lead | leadsignal-loss-second-lead | display changed from left to right
8410584.6 | Lead wire loss third-lead | leadwire-loss-third-lead | display changed from left to right
8410584.7 | Lead signal loss third-lead | leadsignal-loss-third-lead | display changed from left to right
8417752.0 | Battery low | device-battery-low | display changed from left to right
8417752.1 | Sensor malfunction | sensor-malfunction | display changed from left to right
8417752.2 | Not enough blood in sample | sensor-sample-size-insufficient | display changed from left to right
8417752.3 | Sensor strip insertion | sensor-strip-insertion | display changed from left to right
8417752.4 | Sensor strip type incorrect | sensor-strip-type-incorrect | display changed from left to right
8417752.5 | Sensor result too high | sensor-result-too-high | display changed from left to right
8417752.6 | Sensor result too low | sensor-result-too-low | display changed from left to right
8417752.7 | Sensor temp too high | sensor-temp-too-high | display changed from left to right
8417752.8 | Sensor temp too low | sensor-temp-too-low | display changed from left to right
8417752.9 | Sensor read interrupt | sensor-read-interrupt | display changed from left to right
8417752.10 | General Device Fault | device-gen-fault | display changed from left to right
8417752.11 | Sensor temp out of range | sensor-temp-out-of-range | display changed from left to right
8417909.0 | INR device battery low | inr-device-battery-low | display changed from left to right
8417909.1 | Sensor malfunction | inr-sensor-malfunction | display changed from left to right
8417909.2 | Not enough blood in sample | inr-sensor-sample-size-insufficient | display changed from left to right
8417909.3 | INR sensor strip insertion | inr-sensor-strip-insertion | display changed from left to right
8417909.4 | INR sensor strip type incorrect | inr-sensor-strip-type-incorrect | display changed from left to right
8417909.5 | INR sensor result too high | inr-sensor-result-too-high | display changed from left to right
8417909.6 | INR sensor result too low | inr-sensor-result-too-low | display changed from left to right
8417909.7 | INR sensor temp too high | inr-sensor-temp-too-high | display changed from left to right
8417909.8 | INR sensor temp too low | inr-sensor-temp-too-low | display changed from left to right
8417909.9 | INR sensor read interrupt | inr-sensor-read-interrupt | display changed from left to right
8417909.10 | INR device general fault | inr-device-gen-fault | display changed from left to right
8417909.11 | INR sensor calibration due | inr-sensor-calibration-due | display changed from left to right
8408608.0 | Undetermined device status | device-status-undetermined | display changed from left to right
8408608.1 | Device status reset | device-status-reset | display changed from left to right
8408608.5 | Device status error | device-status-error | display changed from left to right
8408608.6 | Device status error mechanical | device-status-error-mechanical | display changed from left to right
8408608.7 | Device status error electronic | device-status-error-electronic | display changed from left to right
8408608.8 | Device status error software | device-status-error-software | display changed from left to right
8408608.9 | Device status error battery | device-status-error-battery | display changed from left to right
8408608.15 | Device status service | device-status-service | display changed from left to right
8408608.16 | Device status service time-sync required | device-status-service-time-sync-required | display changed from left to right
8408608.17 | Device status service calibration required | device-status-service-calibration-required | display changed from left to right
8408608.18 | Device status service replentishment required | device-status-service-replenishment-required | display changed from left to right
8408608.25 | Device status battery low | device-status-battery-low | display changed from left to right
8408608.26 | Device status battery depleted | device-status-battery-depleted | display changed from left to right
8408608.27 | Device status battery replaced | device-status-battery-replaced | display changed from left to right
8408608.28 | Device status battery interrupted | device-status-battery-interrupted | display changed from left to right
8418060.0 | Sensor session stopped | sensor-session-stopped | display changed from left to right
8418060.2 | Sensor type incorrect | sensor-type-incorrect | display changed from left to right
8418060.3 | Sensor malfunction | sensor-malfunction | display changed from left to right
8418060.4 | Device specific alert | device-specific-alert | display changed from left to right
8418060.7 | Sensor calibration not allowed | sensor-calibration-not-allowed | display changed from left to right
8418060.8 | Sensor calibration recommended | sensor-calibration-recommended | display changed from left to right
8418060.9 | Sensor calibration required | sensor-calibration-required | display changed from left to right
8418060.10 | Sensor temp too high | sensor-temp-too-high | display changed from left to right
8418060.11 | Sensor temp too low | sensor-temp-too-low | display changed from left to right
8418060.12 | Sensor result below patient level | sensor-result-below-patient-low | display changed from left to right
8418060.13 | Sensor result above patient level | sensor-result-above-patient-high | display changed from left to right
8418060.14 | Sensor low hypo | sensor-low-hypo | display changed from left to right
8418060.15 | Sensor result hyper | sensor-high-hyper | display changed from left to right
8418060.16 | Sensor rate decrease exceeded | sensor-rate-decrease-exceeded | display changed from left to right
8418060.17 | Sensor rate increase exceeded | sensor-rate-increase-exceeded | display changed from left to right
8418060.18 | Sensor result too low | sensor-result-too-low | display changed from left to right
8418060.19 | Sensor result too high | sensor-result-too-high | display changed from left to right
8418060.20 | Sensor com out of range | sensor-com-out-of-range | display changed from left to right
8418512.0 |  | Battery-status-Undetermined | Added to expansion
8418512.1 |  | Battery-absent | Added to expansion
8418512.2 |  | Battery-active | Added to expansion
8418512.3 |  | Battery-charging | Added to expansion
8418512.4 |  | Battery-fullyCharged | Added to expansion
8418512.5 |  | Battery-disposable | Added to expansion
8418512.6 |  | Battery-rechargeable | Added to expansion
8418512.8 |  | Battery-faulty | Added to expansion
8418512.7 |  | Battery-overTemperature | Added to expansion
8418512.9 |  | Battery-incompatible | Added to expansion
8410608.0 |  | body-movement | Added to expansion
8410608.1 |  | cuff-too-loose | Added to expansion
8410608.2 |  | irregular-pulse | Added to expansion
8410608.3 |  | pulse-over-range-limit | Added to expansion
8410608.4 |  | pulse-under-range-limit | Added to expansion
8410608.5 |  | improper-body-position | Added to expansion