Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## Resource Profile: PhgDevice

Defining URL: | http://hl7.org/fhir/uv/phd/StructureDefinition/PhgDevice
Version: | 1.0.0
Name: | PhgDevice
Status: | Draft as of 2017-07-07 11:39:51-0400
Definition: | Base StructureDefinition for the Device Resource for a PHG
Publisher: | HL7 International - Health Care Devices Work Group
Committee: | Orders and Observations
Source Resource: | XML / JSON / Turtle

The official URL for this profile is:

    http://hl7.org/fhir/uv/phd/StructureDefinition/PhgDevice

### Formal Views of Profile Content

Description of Profiles, Differentials, Snapshots and how the different presentations work.

- Text Summary
- Differential Table
- Snapshot Table
- Snapshot Table (Must Support)
- All

This structure is derived from Device

Summary

Mandatory: 24 elements (38 nested mandatory elements)
Fixed Value: 20 elements
Prohibited: 3 elements

Slices

This structure defines the following Slices:

- The element Device.meta.profile is sliced based on the value of value:value
- The element Device.identifier is sliced based on the values of value:type.coding.system, value:type.coding.code
- The element Device.type.coding is sliced based on the value of value:system
- The element Device.specialization.systemType.coding is sliced based on the value of value:system
- The element Device.version.type.coding is sliced based on the value of value:system
- The element Device.property is sliced based on the value of value:type
- The element Device.property.valueCode.coding is sliced based on the value of value:system

This structure is derived from Device

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
meta |  | 1..1 | Meta | Metadata about the resource
Slices for profile |  | 1..* | canonical(StructureDefinition) | Profiles this resource claims to conform to Slice: Unordered, Open by value:value
profile:phdProfile |  | 1..1 | canonical(StructureDefinition) | Profiles this resource claims to conform to Fixed Value: http://hl7.org/fhir/uv/phd/StructureDefinition/PhgDevice
Slices for identifier |  | 1..* | Identifier | Information that uniquely describes the personal health device Slice: Unordered, Open by value:type.coding.system, value:type.coding.code
identifier:systemIdIdentifier |  | 1..1 | Identifier | System Id identifier
type |  | 1..1 | CodeableConcept | Description of identifier
coding |  | 1..1 | Coding | Indicates this is the IEEE 11073 System Id identifier
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: SYSID
system |  | 1..1 | uri | EUI-64 system identifier Fixed Value: urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680
value |  | 1..1 | string | System id value from System-Id attribute
identifier:btmacAddressIdentifier |  | 0..1 | Identifier | Bluetooth MAC Transport address identifier
type |  | 1..1 | CodeableConcept | Description of identifier
coding |  | 1..1 | Coding | Indicates this is the Bluetooth Mac address identifier
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: BTMAC
system |  | 1..1 | uri | The namespace for the identifier value Fixed Value: http://hl7.org/fhir/sid/eui-48/bluetooth
value |  | 1..1 | string | The value that is unique
identifier:macAddressIdentifier |  | 0..1 | Identifier | MAC Transport address identifier
type |  | 1..1 | CodeableConcept | Description of identifier
coding |  | 1..1 | Coding | Indicates this is the Mac address identifier
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: ETHMAC
system |  | 1..1 | uri | The namespace for the identifier value Fixed Value: http://hl7.org/fhir/sid/eui-48/ethernet
value |  | 1..1 | string | The value that is unique
manufacturer |  | 0..1 | string | Manufacturer name
serialNumber |  | 0..1 | string | Serial number
modelNumber |  | 0..1 | string | Model number
partNumber |  | 0..1 | string | The part number of the device
type |  | 1..1 | CodeableConcept | Indicates the device is a PHG.
Slices for coding |  | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType |  | 1..1 | Coding | Required MDC code system entry
system |  | 1..1 | uri | Identifies IEEE 11073 10101 coding system Fixed Value: urn:iso:std:iso:11073:10101
code |  | 1..1 | code | Indicates PHG Fixed Value: 531981
text |  | 0..1 | string | Plain text representation of the concept
specialization |  | 0..* | BackboneElement | This element contains an entry for each supported specialization or a generic representation
systemType |  | 1..1 | CodeableConcept | The specialization standard supported by the PHG.
Slices for coding |  | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType |  | 1..1 | Coding | Required MDC code system entry for specializations
system |  | 1..1 | uri | The 11073-10101 system identifier Fixed Value: urn:iso:std:iso:11073:10101
code |  | 1..1 | code | The 11073-10101 specialization code. Generic indicates it supports all.
version |  | 0..1 | string | The version of the specialization standard supported by the PHG
version |  | 1..* | BackboneElement | A firmware, hardware, software, internal protocol may be reported for a PHG. A Continua version shall be reported.
type |  | 1..1 | CodeableConcept | The type of the device version
Slices for coding |  | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType |  | 1..1 | Coding | Required MDC code system entry
system |  | 1..1 | uri | Indicates the codes come from the MDC coding system Fixed Value: urn:iso:std:iso:11073:10101
code |  | 1..1 | code | A code indicating the type of version the Device.version.value refers to.
value |  | 1..1 | string | The version
Slices for property |  | 1..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties Slice: Unordered, Open by value:type
property:bitProperties |  | 0..* | BackboneElement | Properties reported in BITs fields
type |  | 1..1 | CodeableConcept | Tells what the BITs item is Binding: ANS1ToHL7 codes defined for non-measurement attributes (required)
coding |  | 1..1 | Coding | Required ASN1 code system entry
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7
code |  | 1..1 | code | Symbol in syntax defined by the system
text |  | 0..1 | string | Plain text representation of the concept
valueQuantity |  | 0..0 |  |
valueCode |  | 1..1 | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
Slices for coding |  | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:V2Binary |  | 1..1 | Coding | Required V2 Binary code system entry
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://terminology.hl7.org/CodeSystem/v2-0136
code |  | 1..1 | code | Symbol in syntax defined by the system
property:quantitiesProperty |  | 0..* | BackboneElement | The PHG properties represented by quantities such as time synchronization accuracy
type |  | 1..1 | CodeableConcept | The type of time quantity Binding: Quantity 11073 Attributes (required)
coding |  | 1..* | Coding | Required MDC code system entry
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: urn:iso:std:iso:11073:10101
code |  | 1..1 | code | Symbol in syntax defined by the system
text |  | 0..1 | string | Plain text representation of the concept
valueQuantity |  | 1..1 | Quantity | Property value as a quantity
value |  | 1..1 | decimal | Numerical value (with implicit precision)
system |  | 1..1 | uri | System that defines coded unit form Fixed Value: http://unitsofmeasure.org
code |  | 1..1 | code | Coded form of the unit Fixed Value: us
valueCode |  | 0..0 |  |
property:codedListProperties |  | 0..* | BackboneElement | The device properties represented by a list of codes such as the list of certified PHD or H-FS interfaces
type |  | 1..1 | CodeableConcept | What the coded list is Binding: CodeableConcept 11073 Attributes (required)
coding |  | 1..* | Coding | Required MDC code system entry
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: urn:iso:std:iso:11073:10101
code |  | 1..1 | code | Symbol in syntax defined by the system
text |  | 0..1 | string | Plain text representation of the concept
valueQuantity |  | 0..0 |  |
valueCode |  | 1..* | CodeableConcept | There shall be one valueCode entry for every item supported by the PHG in the list
coding |  | 1..* | Coding | Code defined by a terminology system
system |  | 1..1 | uri | Identity of the terminology system
code |  | 1..1 | code | Symbol in syntax defined by the system
Documentation for this format

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
id | Σ | 0..1 | string | Logical id of this artifact
meta | Σ | 1..1 | Meta | Metadata about the resource
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
versionId | Σ | 0..1 | id | Version specific identifier
lastUpdated | Σ | 0..1 | instant | When the resource version last changed
source | Σ | 0..1 | uri | Identifies where the resource comes from
Slices for profile | Σ | 1..* | canonical(StructureDefinition) | Profiles this resource claims to conform to Slice: Unordered, Open by value:value
profile:phdProfile | Σ | 1..1 | canonical(StructureDefinition) | Profiles this resource claims to conform to Fixed Value: http://hl7.org/fhir/uv/phd/StructureDefinition/PhgDevice
security | Σ | 0..* | Coding | Security Labels applied to this resource Binding: All Security Labels (extensible): Security Labels from the Healthcare Privacy and Security Classification System.
tag | Σ | 0..* | Coding | Tags applied to this resource Binding: CommonTags (example): Codes that represent various types of tags, commonly workflow-related; e.g. "Needs review by Dr. Jones".
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: CommonLanguages (preferred): A human language.
Additional Bindings | Purpose
AllLanguages | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
Slices for identifier |  | 1..* | Identifier | Information that uniquely describes the personal health device Slice: Unordered, Open by value:type.coding.system, value:type.coding.code
identifier:systemIdIdentifier |  | 1..1 | Identifier | System Id identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
type | Σ | 1..1 | CodeableConcept | Description of identifier Binding: Identifier Type Codes (extensible): A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..1 | Coding | Indicates this is the IEEE 11073 System Id identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system Fixed Value: SYSID
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
system | Σ | 1..1 | uri | EUI-64 system identifier Fixed Value: urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680
value | Σ | 1..1 | string | System id value from System-Id attribute Example General: 123456
period | Σ | 0..1 | Period | Time period when id is/was valid for use
assigner | Σ | 0..1 | Reference(Organization) | Organization that issued id (may be just text)
identifier:btmacAddressIdentifier |  | 0..1 | Identifier | Bluetooth MAC Transport address identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
type | Σ | 1..1 | CodeableConcept | Description of identifier Binding: Identifier Type Codes (extensible): A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..1 | Coding | Indicates this is the Bluetooth Mac address identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system Fixed Value: BTMAC
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
system | Σ | 1..1 | uri | The namespace for the identifier value Fixed Value: http://hl7.org/fhir/sid/eui-48/bluetooth
value | Σ | 1..1 | string | The value that is unique Example General: 123456
period | Σ | 0..1 | Period | Time period when id is/was valid for use
assigner | Σ | 0..1 | Reference(Organization) | Organization that issued id (may be just text)
identifier:macAddressIdentifier |  | 0..1 | Identifier | MAC Transport address identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
type | Σ | 1..1 | CodeableConcept | Description of identifier Binding: Identifier Type Codes (extensible): A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..1 | Coding | Indicates this is the Mac address identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system Fixed Value: ETHMAC
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
system | Σ | 1..1 | uri | The namespace for the identifier value Fixed Value: http://hl7.org/fhir/sid/eui-48/ethernet
value | Σ | 1..1 | string | The value that is unique Example General: 123456
period | Σ | 0..1 | Period | Time period when id is/was valid for use
assigner | Σ | 0..1 | Reference(Organization) | Organization that issued id (may be just text)
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer |  | 0..1 | string | Manufacturer name
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Serial number
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required): The type of name the device is referred by.
modelNumber |  | 0..1 | string | Model number
partNumber |  | 0..1 | string | The part number of the device
type |  | 1..1 | CodeableConcept | Indicates the device is a PHG. Binding: DeviceType (example): Codes to identify medical devices.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
Slices for coding | Σ | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType | Σ | 1..1 | Coding | Required MDC code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identifies IEEE 11073 10101 coding system Fixed Value: urn:iso:std:iso:11073:10101
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Indicates PHG Fixed Value: 531981
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
specialization |  | 0..* | BackboneElement | This element contains an entry for each supported specialization or a generic representation
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The specialization standard supported by the PHG.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
Slices for coding | Σ | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType | Σ | 1..1 | Coding | Required MDC code system entry for specializations
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | The 11073-10101 system identifier Fixed Value: urn:iso:std:iso:11073:10101
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | The 11073-10101 specialization code. Generic indicates it supports all.
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
version |  | 0..1 | string | The version of the specialization standard supported by the PHG
version |  | 1..* | BackboneElement | A firmware, hardware, software, internal protocol may be reported for a PHG. A Continua version shall be reported.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | The type of the device version
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
Slices for coding | Σ | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType | Σ | 1..1 | Coding | Required MDC code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Indicates the codes come from the MDC coding system Fixed Value: urn:iso:std:iso:11073:10101
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | A code indicating the type of version the Device.version.value refers to.
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version
Slices for property |  | 1..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties Slice: Unordered, Open by value:type
property:All Slices |  |  |  | Content/Rules for all slices
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
property:bitProperties |  | 0..* | BackboneElement | Properties reported in BITs fields
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Tells what the BITs item is Binding: ANS1ToHL7 codes defined for non-measurement attributes (required)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..1 | Coding | Required ASN1 code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
valueCode |  | 1..1 | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
Slices for coding | Σ | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:V2Binary | Σ | 1..1 | Coding | Required V2 Binary code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: http://terminology.hl7.org/CodeSystem/v2-0136
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
property:quantitiesProperty |  | 0..* | BackboneElement | The PHG properties represented by quantities such as time synchronization accuracy
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | The type of time quantity Binding: Quantity 11073 Attributes (required)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..* | Coding | Required MDC code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: urn:iso:std:iso:11073:10101
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
valueQuantity |  | 1..1 | Quantity | Property value as a quantity
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
value | Σ | 1..1 | decimal | Numerical value (with implicit precision)
comparator | ?!Σ | 0..1 | code | < | <= | >= | > - how to understand the value Binding: QuantityComparator (required): How the Quantity should be understood and represented.
unit | Σ | 0..1 | string | Unit representation
system | Σ I | 1..1 | uri | System that defines coded unit form Fixed Value: http://unitsofmeasure.org
code | Σ | 1..1 | code | Coded form of the unit Fixed Value: us
property:codedListProperties |  | 0..* | BackboneElement | The device properties represented by a list of codes such as the list of certified PHD or H-FS interfaces
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | What the coded list is Binding: CodeableConcept 11073 Attributes (required)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..* | Coding | Required MDC code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: urn:iso:std:iso:11073:10101
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
valueCode |  | 1..* | CodeableConcept | There shall be one valueCode entry for every item supported by the PHG in the list
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..* | Coding | Code defined by a terminology system
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device
parent |  | 0..1 | Reference(Device) | The parent device
Documentation for this format

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
Documentation for this format

This structure is derived from Device

Summary

Mandatory: 24 elements (38 nested mandatory elements)
Fixed Value: 20 elements
Prohibited: 3 elements

Slices

This structure defines the following Slices:

- The element Device.meta.profile is sliced based on the value of value:value
- The element Device.identifier is sliced based on the values of value:type.coding.system, value:type.coding.code
- The element Device.type.coding is sliced based on the value of value:system
- The element Device.specialization.systemType.coding is sliced based on the value of value:system
- The element Device.version.type.coding is sliced based on the value of value:system
- The element Device.property is sliced based on the value of value:type
- The element Device.property.valueCode.coding is sliced based on the value of value:system

Differential View

This structure is derived from Device

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
meta |  | 1..1 | Meta | Metadata about the resource
Slices for profile |  | 1..* | canonical(StructureDefinition) | Profiles this resource claims to conform to Slice: Unordered, Open by value:value
profile:phdProfile |  | 1..1 | canonical(StructureDefinition) | Profiles this resource claims to conform to Fixed Value: http://hl7.org/fhir/uv/phd/StructureDefinition/PhgDevice
Slices for identifier |  | 1..* | Identifier | Information that uniquely describes the personal health device Slice: Unordered, Open by value:type.coding.system, value:type.coding.code
identifier:systemIdIdentifier |  | 1..1 | Identifier | System Id identifier
type |  | 1..1 | CodeableConcept | Description of identifier
coding |  | 1..1 | Coding | Indicates this is the IEEE 11073 System Id identifier
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: SYSID
system |  | 1..1 | uri | EUI-64 system identifier Fixed Value: urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680
value |  | 1..1 | string | System id value from System-Id attribute
identifier:btmacAddressIdentifier |  | 0..1 | Identifier | Bluetooth MAC Transport address identifier
type |  | 1..1 | CodeableConcept | Description of identifier
coding |  | 1..1 | Coding | Indicates this is the Bluetooth Mac address identifier
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: BTMAC
system |  | 1..1 | uri | The namespace for the identifier value Fixed Value: http://hl7.org/fhir/sid/eui-48/bluetooth
value |  | 1..1 | string | The value that is unique
identifier:macAddressIdentifier |  | 0..1 | Identifier | MAC Transport address identifier
type |  | 1..1 | CodeableConcept | Description of identifier
coding |  | 1..1 | Coding | Indicates this is the Mac address identifier
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
code |  | 1..1 | code | Symbol in syntax defined by the system Fixed Value: ETHMAC
system |  | 1..1 | uri | The namespace for the identifier value Fixed Value: http://hl7.org/fhir/sid/eui-48/ethernet
value |  | 1..1 | string | The value that is unique
manufacturer |  | 0..1 | string | Manufacturer name
serialNumber |  | 0..1 | string | Serial number
modelNumber |  | 0..1 | string | Model number
partNumber |  | 0..1 | string | The part number of the device
type |  | 1..1 | CodeableConcept | Indicates the device is a PHG.
Slices for coding |  | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType |  | 1..1 | Coding | Required MDC code system entry
system |  | 1..1 | uri | Identifies IEEE 11073 10101 coding system Fixed Value: urn:iso:std:iso:11073:10101
code |  | 1..1 | code | Indicates PHG Fixed Value: 531981
text |  | 0..1 | string | Plain text representation of the concept
specialization |  | 0..* | BackboneElement | This element contains an entry for each supported specialization or a generic representation
systemType |  | 1..1 | CodeableConcept | The specialization standard supported by the PHG.
Slices for coding |  | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType |  | 1..1 | Coding | Required MDC code system entry for specializations
system |  | 1..1 | uri | The 11073-10101 system identifier Fixed Value: urn:iso:std:iso:11073:10101
code |  | 1..1 | code | The 11073-10101 specialization code. Generic indicates it supports all.
version |  | 0..1 | string | The version of the specialization standard supported by the PHG
version |  | 1..* | BackboneElement | A firmware, hardware, software, internal protocol may be reported for a PHG. A Continua version shall be reported.
type |  | 1..1 | CodeableConcept | The type of the device version
Slices for coding |  | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType |  | 1..1 | Coding | Required MDC code system entry
system |  | 1..1 | uri | Indicates the codes come from the MDC coding system Fixed Value: urn:iso:std:iso:11073:10101
code |  | 1..1 | code | A code indicating the type of version the Device.version.value refers to.
value |  | 1..1 | string | The version
Slices for property |  | 1..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties Slice: Unordered, Open by value:type
property:bitProperties |  | 0..* | BackboneElement | Properties reported in BITs fields
type |  | 1..1 | CodeableConcept | Tells what the BITs item is Binding: ANS1ToHL7 codes defined for non-measurement attributes (required)
coding |  | 1..1 | Coding | Required ASN1 code system entry
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7
code |  | 1..1 | code | Symbol in syntax defined by the system
text |  | 0..1 | string | Plain text representation of the concept
valueQuantity |  | 0..0 |  |
valueCode |  | 1..1 | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
Slices for coding |  | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:V2Binary |  | 1..1 | Coding | Required V2 Binary code system entry
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: http://terminology.hl7.org/CodeSystem/v2-0136
code |  | 1..1 | code | Symbol in syntax defined by the system
property:quantitiesProperty |  | 0..* | BackboneElement | The PHG properties represented by quantities such as time synchronization accuracy
type |  | 1..1 | CodeableConcept | The type of time quantity Binding: Quantity 11073 Attributes (required)
coding |  | 1..* | Coding | Required MDC code system entry
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: urn:iso:std:iso:11073:10101
code |  | 1..1 | code | Symbol in syntax defined by the system
text |  | 0..1 | string | Plain text representation of the concept
valueQuantity |  | 1..1 | Quantity | Property value as a quantity
value |  | 1..1 | decimal | Numerical value (with implicit precision)
system |  | 1..1 | uri | System that defines coded unit form Fixed Value: http://unitsofmeasure.org
code |  | 1..1 | code | Coded form of the unit Fixed Value: us
valueCode |  | 0..0 |  |
property:codedListProperties |  | 0..* | BackboneElement | The device properties represented by a list of codes such as the list of certified PHD or H-FS interfaces
type |  | 1..1 | CodeableConcept | What the coded list is Binding: CodeableConcept 11073 Attributes (required)
coding |  | 1..* | Coding | Required MDC code system entry
system |  | 1..1 | uri | Identity of the terminology system Fixed Value: urn:iso:std:iso:11073:10101
code |  | 1..1 | code | Symbol in syntax defined by the system
text |  | 0..1 | string | Plain text representation of the concept
valueQuantity |  | 0..0 |  |
valueCode |  | 1..* | CodeableConcept | There shall be one valueCode entry for every item supported by the PHG in the list
coding |  | 1..* | Coding | Code defined by a terminology system
system |  | 1..1 | uri | Identity of the terminology system
code |  | 1..1 | code | Symbol in syntax defined by the system
Documentation for this format

Snapshot View

Name | Flags | Card. | Type | Description & Constraints
--- | --- | --- | --- | ---
Device |  | 0..* | Device | Item used in healthcare
id | Σ | 0..1 | string | Logical id of this artifact
meta | Σ | 1..1 | Meta | Metadata about the resource
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
versionId | Σ | 0..1 | id | Version specific identifier
lastUpdated | Σ | 0..1 | instant | When the resource version last changed
source | Σ | 0..1 | uri | Identifies where the resource comes from
Slices for profile | Σ | 1..* | canonical(StructureDefinition) | Profiles this resource claims to conform to Slice: Unordered, Open by value:value
profile:phdProfile | Σ | 1..1 | canonical(StructureDefinition) | Profiles this resource claims to conform to Fixed Value: http://hl7.org/fhir/uv/phd/StructureDefinition/PhgDevice
security | Σ | 0..* | Coding | Security Labels applied to this resource Binding: All Security Labels (extensible): Security Labels from the Healthcare Privacy and Security Classification System.
tag | Σ | 0..* | Coding | Tags applied to this resource Binding: CommonTags (example): Codes that represent various types of tags, commonly workflow-related; e.g. "Needs review by Dr. Jones".
implicitRules | ?!Σ | 0..1 | uri | A set of rules under which this content was created
language |  | 0..1 | code | Language of the resource content Binding: CommonLanguages (preferred): A human language.
Additional Bindings | Purpose
AllLanguages | Max Binding
text |  | 0..1 | Narrative | Text summary of the resource, for human interpretation
contained |  | 0..* | Resource | Contained, inline Resources
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?! | 0..* | Extension | Extensions that cannot be ignored
Slices for identifier |  | 1..* | Identifier | Information that uniquely describes the personal health device Slice: Unordered, Open by value:type.coding.system, value:type.coding.code
identifier:systemIdIdentifier |  | 1..1 | Identifier | System Id identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
type | Σ | 1..1 | CodeableConcept | Description of identifier Binding: Identifier Type Codes (extensible): A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..1 | Coding | Indicates this is the IEEE 11073 System Id identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system Fixed Value: SYSID
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
system | Σ | 1..1 | uri | EUI-64 system identifier Fixed Value: urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680
value | Σ | 1..1 | string | System id value from System-Id attribute Example General: 123456
period | Σ | 0..1 | Period | Time period when id is/was valid for use
assigner | Σ | 0..1 | Reference(Organization) | Organization that issued id (may be just text)
identifier:btmacAddressIdentifier |  | 0..1 | Identifier | Bluetooth MAC Transport address identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
type | Σ | 1..1 | CodeableConcept | Description of identifier Binding: Identifier Type Codes (extensible): A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..1 | Coding | Indicates this is the Bluetooth Mac address identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system Fixed Value: BTMAC
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
system | Σ | 1..1 | uri | The namespace for the identifier value Fixed Value: http://hl7.org/fhir/sid/eui-48/bluetooth
value | Σ | 1..1 | string | The value that is unique Example General: 123456
period | Σ | 0..1 | Period | Time period when id is/was valid for use
assigner | Σ | 0..1 | Reference(Organization) | Organization that issued id (may be just text)
identifier:macAddressIdentifier |  | 0..1 | Identifier | MAC Transport address identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
use | ?!Σ | 0..1 | code | usual | official | temp | secondary | old (If known) Binding: IdentifierUse (required): Identifies the purpose for this identifier, if known .
type | Σ | 1..1 | CodeableConcept | Description of identifier Binding: Identifier Type Codes (extensible): A coded type for an identifier that can be used to determine which identifier to use for a specific purpose.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..1 | Coding | Indicates this is the Mac address identifier
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system Fixed Value: ETHMAC
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
system | Σ | 1..1 | uri | The namespace for the identifier value Fixed Value: http://hl7.org/fhir/sid/eui-48/ethernet
value | Σ | 1..1 | string | The value that is unique Example General: 123456
period | Σ | 0..1 | Period | Time period when id is/was valid for use
assigner | Σ | 0..1 | Reference(Organization) | Organization that issued id (may be just text)
definition |  | 0..1 | Reference(DeviceDefinition) | The reference to the definition for the device
udiCarrier | Σ | 0..* | BackboneElement | Unique Device Identifier (UDI) Barcode string
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
deviceIdentifier | Σ | 0..1 | string | Mandatory fixed portion of UDI
issuer |  | 0..1 | uri | UDI Issuing Organization
jurisdiction |  | 0..1 | uri | Regional UDI authority
carrierAIDC | Σ | 0..1 | base64Binary | UDI Machine Readable Barcode String
carrierHRF | Σ | 0..1 | string | UDI Human Readable Barcode String
entryType |  | 0..1 | code | barcode | rfid | manual + Binding: UDIEntryType (required): Codes to identify how UDI data was entered.
status | ?!Σ | 0..1 | code | active | inactive | entered-in-error | unknown Binding: FHIRDeviceStatus (required): The availability status of the device.
statusReason |  | 0..* | CodeableConcept | online | paused | standby | offline | not-ready | transduc-discon | hw-discon | off Binding: FHIRDeviceStatusReason (extensible): The availability status reason of the device.
distinctIdentifier |  | 0..1 | string | The distinct identification string
manufacturer |  | 0..1 | string | Manufacturer name
manufactureDate |  | 0..1 | dateTime | Date when the device was made
expirationDate |  | 0..1 | dateTime | Date and time of expiry of this device (if applicable)
lotNumber |  | 0..1 | string | Lot number of manufacture
serialNumber |  | 0..1 | string | Serial number
deviceName |  | 0..* | BackboneElement | The name of the device as given by the manufacturer
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
name |  | 1..1 | string | The name of the device
type |  | 1..1 | code | udi-label-name | user-friendly-name | patient-reported-name | manufacturer-name | model-name | other Binding: DeviceNameType (required): The type of name the device is referred by.
modelNumber |  | 0..1 | string | Model number
partNumber |  | 0..1 | string | The part number of the device
type |  | 1..1 | CodeableConcept | Indicates the device is a PHG. Binding: DeviceType (example): Codes to identify medical devices.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
Slices for coding | Σ | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType | Σ | 1..1 | Coding | Required MDC code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identifies IEEE 11073 10101 coding system Fixed Value: urn:iso:std:iso:11073:10101
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Indicates PHG Fixed Value: 531981
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
specialization |  | 0..* | BackboneElement | This element contains an entry for each supported specialization or a generic representation
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
systemType |  | 1..1 | CodeableConcept | The specialization standard supported by the PHG.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
Slices for coding | Σ | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType | Σ | 1..1 | Coding | Required MDC code system entry for specializations
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | The 11073-10101 system identifier Fixed Value: urn:iso:std:iso:11073:10101
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | The 11073-10101 specialization code. Generic indicates it supports all.
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
version |  | 0..1 | string | The version of the specialization standard supported by the PHG
version |  | 1..* | BackboneElement | A firmware, hardware, software, internal protocol may be reported for a PHG. A Continua version shall be reported.
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | The type of the device version
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
Slices for coding | Σ | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:MDCType | Σ | 1..1 | Coding | Required MDC code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Indicates the codes come from the MDC coding system Fixed Value: urn:iso:std:iso:11073:10101
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | A code indicating the type of version the Device.version.value refers to.
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
component |  | 0..1 | Identifier | A single component of the device version
value |  | 1..1 | string | The version
Slices for property |  | 1..* | BackboneElement | The actual configuration settings of a device as it actually operates, e.g., regulation status, time properties Slice: Unordered, Open by value:type
property:All Slices |  |  |  | Content/Rules for all slices
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Code that specifies the property DeviceDefinitionPropetyCode (Extensible)
valueQuantity |  | 0..* | Quantity | Property value as a quantity
valueCode |  | 0..* | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
property:bitProperties |  | 0..* | BackboneElement | Properties reported in BITs fields
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | Tells what the BITs item is Binding: ANS1ToHL7 codes defined for non-measurement attributes (required)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..1 | Coding | Required ASN1 code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
valueCode |  | 1..1 | CodeableConcept | Property value as a code, e.g., NTP4 (synced to NTP)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
Slices for coding | Σ | 1..* | Coding | Code defined by a terminology system Slice: Unordered, Open by value:system
coding:V2Binary | Σ | 1..1 | Coding | Required V2 Binary code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: http://terminology.hl7.org/CodeSystem/v2-0136
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
property:quantitiesProperty |  | 0..* | BackboneElement | The PHG properties represented by quantities such as time synchronization accuracy
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | The type of time quantity Binding: Quantity 11073 Attributes (required)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..* | Coding | Required MDC code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: urn:iso:std:iso:11073:10101
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
valueQuantity |  | 1..1 | Quantity | Property value as a quantity
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
value | Σ | 1..1 | decimal | Numerical value (with implicit precision)
comparator | ?!Σ | 0..1 | code | < | <= | >= | > - how to understand the value Binding: QuantityComparator (required): How the Quantity should be understood and represented.
unit | Σ | 0..1 | string | Unit representation
system | Σ I | 1..1 | uri | System that defines coded unit form Fixed Value: http://unitsofmeasure.org
code | Σ | 1..1 | code | Coded form of the unit Fixed Value: us
property:codedListProperties |  | 0..* | BackboneElement | The device properties represented by a list of codes such as the list of certified PHD or H-FS interfaces
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations
modifierExtension | ?!Σ | 0..* | Extension | Extensions that cannot be ignored even if unrecognized
type |  | 1..1 | CodeableConcept | What the coded list is Binding: CodeableConcept 11073 Attributes (required)
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..* | Coding | Required MDC code system entry
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system Fixed Value: urn:iso:std:iso:11073:10101
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
valueCode |  | 1..* | CodeableConcept | There shall be one valueCode entry for every item supported by the PHG in the list
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
coding | Σ | 1..* | Coding | Code defined by a terminology system
id |  | 0..1 | string | Unique id for inter-element referencing
extension |  | 0..* | Extension | Additional content defined by implementations Slice: Unordered, Open by value:url
system | Σ | 1..1 | uri | Identity of the terminology system
version | Σ | 0..1 | string | Version of the system - if relevant
code | Σ | 1..1 | code | Symbol in syntax defined by the system
display | Σ | 0..1 | string | Representation defined by the system
userSelected | Σ | 0..1 | boolean | If this coding was chosen directly by the user
text | Σ | 0..1 | string | Plain text representation of the concept
patient |  | 0..1 | Reference(Patient) | Patient to whom Device is affixed
owner |  | 0..1 | Reference(Organization) | Organization responsible for device
contact |  | 0..* | ContactPoint | Details for human/organization for support
location |  | 0..1 | Reference(Location) | Where the device is found
url |  | 0..1 | uri | Network address to contact device
note |  | 0..* | Annotation | Device notes and comments
safety | Σ | 0..* | CodeableConcept | Safety Characteristics of Device
parent |  | 0..1 | Reference(Device) | The parent device
Documentation for this format

Other representations of profile: CSV, Excel, Schematron

#### Terminology Bindings

Path | Conformance | ValueSet
Device.meta.security | extensible | All Security Labels
Device.meta.tag | example | CommonTags
Device.language | preferred | CommonLanguages Max Binding: AllLanguages
Device.identifier:systemIdIdentifier.use | required | IdentifierUse
Device.identifier:systemIdIdentifier.type | extensible | Identifier Type Codes
Device.identifier:btmacAddressIdentifier.use | required | IdentifierUse
Device.identifier:btmacAddressIdentifier.type | extensible | Identifier Type Codes
Device.identifier:macAddressIdentifier.use | required | IdentifierUse
Device.identifier:macAddressIdentifier.type | extensible | Identifier Type Codes
Device.udiCarrier.entryType | required | UDIEntryType
Device.status | required | FHIRDeviceStatus
Device.statusReason | extensible | FHIRDeviceStatusReason
Device.deviceName.type | required | DeviceNameType
Device.type | example | DeviceType
Device.property:bitProperties.type | required | ASN1attribute
Device.property:quantitiesProperty.type | required | Quantity11073MDC
Device.property:quantitiesProperty.valueQuantity.comparator | required | QuantityComparator
Device.property:codedListProperties.type | required | CodeableConcept11073MDC

#### Constraints

Id | Grade | Path | Details | Requirements
dom-2 | error | Device | If the resource is contained in another resource, it SHALL NOT contain nested Resources : contained.contained.empty() |
dom-3 | error | Device | If the resource is contained in another resource, it SHALL be referred to from elsewhere in the resource or SHALL refer to the containing resource : contained.where((('#'+id in (%resource.descendants().reference | %resource.descendants().as(canonical) | %resource.descendants().as(uri) | %resource.descendants().as(url))) or descendants().where(reference = '#').exists() or descendants().where(as(canonical) = '#').exists() or descendants().where(as(canonical) = '#').exists()).not()).trace('unmatched', id).empty() |
dom-4 | error | Device | If a resource is contained in another resource, it SHALL NOT have a meta.versionId or a meta.lastUpdated : contained.meta.versionId.empty() and contained.meta.lastUpdated.empty() |
dom-5 | error | Device | If a resource is contained in another resource, it SHALL NOT have a security label : contained.meta.security.empty() |
dom-6 | Best Practice | Device | A resource should have narrative for robust management : text.`div`.exists() |
ele-1 | error | Device.meta | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.meta.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.meta.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.meta.versionId | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.meta.lastUpdated | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.meta.source | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.meta.profile | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.meta.profile:phdProfile | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.meta.security | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.meta.tag | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.implicitRules | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.language | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.modifierExtension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.modifierExtension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.identifier | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.identifier:systemIdIdentifier.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.identifier:systemIdIdentifier.use | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.type | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.type.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.identifier:systemIdIdentifier.type.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.identifier:systemIdIdentifier.type.coding | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.type.coding.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.identifier:systemIdIdentifier.type.coding.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.identifier:systemIdIdentifier.type.coding.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.type.coding.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.type.coding.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.type.coding.display | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.type.coding.userSelected | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.type.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.value | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.period | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:systemIdIdentifier.assigner | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.identifier:btmacAddressIdentifier.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.identifier:btmacAddressIdentifier.use | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.type | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.type.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.identifier:btmacAddressIdentifier.type.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.identifier:btmacAddressIdentifier.type.coding | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.type.coding.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.identifier:btmacAddressIdentifier.type.coding.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.identifier:btmacAddressIdentifier.type.coding.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.type.coding.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.type.coding.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.type.coding.display | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.type.coding.userSelected | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.type.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.value | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.period | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:btmacAddressIdentifier.assigner | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.identifier:macAddressIdentifier.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.identifier:macAddressIdentifier.use | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.type | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.type.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.identifier:macAddressIdentifier.type.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.identifier:macAddressIdentifier.type.coding | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.type.coding.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.identifier:macAddressIdentifier.type.coding.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.identifier:macAddressIdentifier.type.coding.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.type.coding.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.type.coding.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.type.coding.display | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.type.coding.userSelected | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.type.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.value | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.period | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.identifier:macAddressIdentifier.assigner | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.definition | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.udiCarrier | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.udiCarrier.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.udiCarrier.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.udiCarrier.modifierExtension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.udiCarrier.modifierExtension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.udiCarrier.deviceIdentifier | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.udiCarrier.issuer | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.udiCarrier.jurisdiction | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.udiCarrier.carrierAIDC | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.udiCarrier.carrierHRF | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.udiCarrier.entryType | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.status | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.statusReason | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.distinctIdentifier | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.manufacturer | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.manufactureDate | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.expirationDate | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.lotNumber | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.serialNumber | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.deviceName | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.deviceName.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.deviceName.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.deviceName.modifierExtension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.deviceName.modifierExtension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.deviceName.name | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.deviceName.type | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.modelNumber | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.partNumber | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.type | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.type.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.type.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.type.coding | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.type.coding:MDCType | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.type.coding:MDCType.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.type.coding:MDCType.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.type.coding:MDCType.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.type.coding:MDCType.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.type.coding:MDCType.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.type.coding:MDCType.display | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.type.coding:MDCType.userSelected | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.type.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.specialization | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.specialization.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.specialization.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.specialization.modifierExtension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.specialization.modifierExtension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.specialization.systemType | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.specialization.systemType.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.specialization.systemType.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.specialization.systemType.coding | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.specialization.systemType.coding:MDCType | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.specialization.systemType.coding:MDCType.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.specialization.systemType.coding:MDCType.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.specialization.systemType.coding:MDCType.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.specialization.systemType.coding:MDCType.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.specialization.systemType.coding:MDCType.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.specialization.systemType.coding:MDCType.display | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.specialization.systemType.coding:MDCType.userSelected | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.specialization.systemType.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.specialization.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.version.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.version.modifierExtension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.version.modifierExtension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.version.type | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version.type.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.version.type.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.version.type.coding | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version.type.coding:MDCType | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version.type.coding:MDCType.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.version.type.coding:MDCType.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.version.type.coding:MDCType.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version.type.coding:MDCType.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version.type.coding:MDCType.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version.type.coding:MDCType.display | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version.type.coding:MDCType.userSelected | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version.type.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version.component | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.version.value | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property.modifierExtension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property.modifierExtension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property.type | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property.valueQuantity | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property.valueCode | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:bitProperties.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:bitProperties.modifierExtension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:bitProperties.modifierExtension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:bitProperties.type | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.type.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:bitProperties.type.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:bitProperties.type.coding | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.type.coding.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:bitProperties.type.coding.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:bitProperties.type.coding.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.type.coding.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.type.coding.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.type.coding.display | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.type.coding.userSelected | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.type.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.valueCode | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.valueCode.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:bitProperties.valueCode.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:bitProperties.valueCode.coding | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.valueCode.coding:V2Binary | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.valueCode.coding:V2Binary.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:bitProperties.valueCode.coding:V2Binary.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:bitProperties.valueCode.coding:V2Binary.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.valueCode.coding:V2Binary.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.valueCode.coding:V2Binary.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.valueCode.coding:V2Binary.display | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.valueCode.coding:V2Binary.userSelected | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:bitProperties.valueCode.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:quantitiesProperty.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:quantitiesProperty.modifierExtension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:quantitiesProperty.modifierExtension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:quantitiesProperty.type | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.type.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:quantitiesProperty.type.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:quantitiesProperty.type.coding | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.type.coding.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:quantitiesProperty.type.coding.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:quantitiesProperty.type.coding.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.type.coding.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.type.coding.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.type.coding.display | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.type.coding.userSelected | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.type.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.valueQuantity | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.valueQuantity.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:quantitiesProperty.valueQuantity.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:quantitiesProperty.valueQuantity.value | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.valueQuantity.comparator | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.valueQuantity.unit | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.valueQuantity.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:quantitiesProperty.valueQuantity.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:codedListProperties.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:codedListProperties.modifierExtension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:codedListProperties.modifierExtension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:codedListProperties.type | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.type.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:codedListProperties.type.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:codedListProperties.type.coding | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.type.coding.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:codedListProperties.type.coding.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:codedListProperties.type.coding.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.type.coding.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.type.coding.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.type.coding.display | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.type.coding.userSelected | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.type.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.valueCode | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.valueCode.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:codedListProperties.valueCode.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:codedListProperties.valueCode.coding | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.valueCode.coding.extension | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ext-1 | error | Device.property:codedListProperties.valueCode.coding.extension | Must have either extensions or value[x], not both : extension.exists() != value.exists() |
ele-1 | error | Device.property:codedListProperties.valueCode.coding.system | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.valueCode.coding.version | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.valueCode.coding.code | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.valueCode.coding.display | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.valueCode.coding.userSelected | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.property:codedListProperties.valueCode.text | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.patient | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.owner | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.contact | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.location | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.url | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.note | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.safety | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |
ele-1 | error | Device.parent | All FHIR elements must have a @value or children : hasValue() or (children().count() > id.count()) |