Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## : ContinuaDeviceIdentifiers - JSON Representation

Raw json | Download

    {
      "resourceType" : "CodeSystem",
      "id" : "ContinuaDeviceIdentifiers",
      "meta" : {
        "profile" : [
          "http://hl7.org/fhir/StructureDefinition/shareablecodesystem"
        ]
      },
      "text" : {
        "status" : "generated",
        "div" : "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p>This code system http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers defines the following codes:</p><table class=\"codes\"><tr><td style=\"white-space:nowrap\"><b>Code</b></td><td><b>Display</b></td><td><b>Definition</b></td></tr><tr><td style=\"white-space:nowrap\">SYSID<a name=\"ContinuaDeviceIdentifiers-SYSID\"> </a></td><td>IEEE 11073 System Identifier</td><td>This code indicates that the identifier is the IEEE 11073 SystemId from the equivalent of the System-Id attribute</td></tr><tr><td style=\"white-space:nowrap\">BTMAC<a name=\"ContinuaDeviceIdentifiers-BTMAC\"> </a></td><td>Bluetooth MAC address</td><td>This code indicates that the identifier is the Bluetooth MAC address, either classic or low energy</td></tr><tr><td style=\"white-space:nowrap\">ETHMAC<a name=\"ContinuaDeviceIdentifiers-ETHMAC\"> </a></td><td>Ethernet MAC address</td><td>This code indicates that the identifier is the Ethernet MAC address</td></tr><tr><td style=\"white-space:nowrap\">USB<a name=\"ContinuaDeviceIdentifiers-USB\"> </a></td><td>USB PID and VID designators</td><td>This code indicates that the identifier is the USB Pid and Vid values</td></tr><tr><td style=\"white-space:nowrap\">ZIGBEE<a name=\"ContinuaDeviceIdentifiers-ZIGBEE\"> </a></td><td>ZigBee MAC address</td><td>This code indicates that the identifier is the ZigBee MAC address</td></tr></table></div>"
      },
      "url" : "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers",
      "version" : "1.0.0",
      "name" : "ContinuaDeviceIdentifiers",
      "status" : "draft",
      "experimental" : true,
      "date" : "2018-11-25",
      "publisher" : "HL7 International - Health Care Devices Work Group",
      "contact" : [
        {
          "telecom" : [
            {
              "system" : "url",
              "value" : "http://hl7.org/Special/committees/healthcaredevices"
            }
          ]
        }
      ],
      "description" : "Codes used to describe the Device (PHD or PHG) Identifiers, such as the system id or Bluetooth Address. More codes maybe added to this list in the future.",
      "jurisdiction" : [
        {
          "coding" : [
            {
              "system" : "http://unstats.un.org/unsd/methods/m49/m49.htm",
              "code" : "001"
            }
          ]
        }
      ],
      "caseSensitive" : true,
      "hierarchyMeaning" : "grouped-by",
      "content" : "complete",
      "concept" : [
        {
          "code" : "SYSID",
          "display" : "IEEE 11073 System Identifier",
          "definition" : "This code indicates that the identifier is the IEEE 11073 SystemId from the equivalent of the System-Id attribute"
        },
        {
          "code" : "BTMAC",
          "display" : "Bluetooth MAC address",
          "definition" : "This code indicates that the identifier is the Bluetooth MAC address, either classic or low energy"
        },
        {
          "code" : "ETHMAC",
          "display" : "Ethernet MAC address",
          "definition" : "This code indicates that the identifier is the Ethernet MAC address"
        },
        {
          "code" : "USB",
          "display" : "USB PID and VID designators",
          "definition" : "This code indicates that the identifier is the USB Pid and Vid values"
        },
        {
          "code" : "ZIGBEE",
          "display" : "ZigBee MAC address",
          "definition" : "This code indicates that the identifier is the ZigBee MAC address"
        }
      ]
    }