Radiation Dose Summary for Diagnostic Procedures on FHIR
0.1.0 - STU 1 Ballot

Publication Build: This will be filled in by the publication tooling

## ValueSet: Irradiation Event component type

Summary

Defining URL: | http://hl7.org/fhir/uv/radiation-dose-summary/ValueSet/component-irradiation-event-vs
Version: | 0.1.0
Name: | ComponentIrradiationEventVS
Title: | Irradiation Event component type
Status: | Active as of 12/8/21 3:51 PM
Definition: | Value Set describing the list of minimal dose information related to irradiation event level
Publisher: | HL7 Imaging Integration Working Group
Source Resource: | XML / JSON / Turtle

References

- CT Irradiation Event Summary
- Irradiation Event Summary

### Logical Definition (CLD)

- Include these codes as defined in `http://dicom.nema.org/resources/ontology/DCM`

  Code | Display
  113838 | DLP
  113830 | Mean CTDIvol
  113835 | CTDIw Phantom Type

### Expansion

This value set contains 3 concepts

Expansion based on DICOM version 01

All codes in this table are from the system `http://dicom.nema.org/resources/ontology/DCM`

Code | Display | Definition
113838 | DLP |
113830 | Mean CTDIvol |
113835 | CTDIw Phantom Type |

Explanation of the columns that may appear on this page:

Level | A few code lists that FHIR defines are hierarchical - each code is assigned a level. In this scheme, some codes are under other codes, and imply that the code they are under also applies
Source | The source of the definition of the code (when the value set draws in codes defined elsewhere)
Code | The code (used as the code in the resource instance)
Display | The display (used in the display element of a Coding). If there is no display, implementers should not simply display the code, but map the concept into their application
Definition | An explanation of the meaning of the concept
Comments | Additional notes about how to use the code