HL7 Version 2 to FHIR
1.0.0 - STU 1

HL7 Version 2 to FHIR - Downloaded Version 1.0.0 See the Directory of published versions

## ConceptMap: Datatype TQ [Priority] to Task Map (Experimental)

Official URL: http://hl7.org/fhir/uv/v2mappings/ConceptMap/datatype-tq-priority-to-task | Version: 1.0.0
Standards status: Informative | Computable Name: DatatypeTQPriorityToTask
Copyright/Legal: Copyright (c) 2025, HL7 International, Inc., All Rights Reserved.

This ConceptMap represents a mapping from the HL7 V2 Datatype TQ to the FHIR Task Resource.

This ConceptMap represents the mapping from the HL7 V2 TQ Data Type to the FHIR Task Resource. See also the FHIR Shorthand or the CSV Source.

HL7 v2 | Condition (IF True, args) | HL7 FHIR | Comments
--- | --- | --- | ---
Sort Order | Identifier | Name | Data Type | Cardinality - Min | Cardinality - Max | Computable ANTLR | Computable FHIRPath | Narrative | FHIR Attribute | Proposed Extension | Data Type | Cardinality - Min | Cardinality - Max | Data Type Mapping | Vocabulary Mapping (IS, ID, CE, CEN, CWE) | Assignment
1 | TQ.1 | Quantity | CQ | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
2 | TQ.2 | Interval | RI | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
3 | TQ.3 | Duration | ST | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
3 | TQ.3 | Duration | ST | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
4 | TQ.4 | Start Date/Time | TS | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
5 | TQ.5 | End Date/Time | TS | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
6 | TQ.6 | Priority | ST | 0 | 1 |  |  |  | Task.priority |  | code | 0 | 1 |  | ExtendedPriorityCodes |  | A translation from the text priority in the v2 message to a coded value in the request-priority value set will be required.
7 | TQ.7 | Condition | ST | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
8 | TQ.8 | Text | TX | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
9 | TQ.9 | Conjunction | ID | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
10 | TQ.10 | Order Sequencing | OSD | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
11 | TQ.11 | Occurrence Duration | CE | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
12 | TQ.12 | Total Occurrences | NM | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |

Mapping from (not specified) to (not specified)

Group 1 Mapping from `unspecified code system` to `unspecified code system`

Source Code | Relationship | Target Code | Comment
TQ.6 (Priority) | is equivalent to | priority | A translation from the text priority in the v2 message to a coded value in the request-priority value set will be required.

### Notes: