HL7 Version 2 to FHIR
1.0.0 - STU 1

HL7 Version 2 to FHIR - Downloaded Version 1.0.0 See the Directory of published versions

## ConceptMap: Datatype RPT to Timing Map (Experimental)

Official URL: http://hl7.org/fhir/uv/v2mappings/ConceptMap/datatype-rpt-to-timing | Version: 1.0.0
Standards status: Informative | Computable Name: DatatypeRPTToTiming
Copyright/Legal: Copyright (c) 2025, HL7 International, Inc., All Rights Reserved.

This ConceptMap represents a mapping from the HL7 V2 Datatype RPT to the FHIR Timing Data Type.

This ConceptMap represents the mapping from the HL7 V2 RPT Data Type to the FHIR Timing Data Type. See also the FHIR Shorthand or the CSV Source.

HL7 v2 | Condition (IF True, args) | HL7 FHIR | Comments
--- | --- | --- | ---
Sort Order | Identifier | Name | Data Type | Cardinality - Min | Cardinality - Max | Computable ANTLR | Computable FHIRPath | Narrative | FHIR Attribute | Proposed Extension | Data Type | Cardinality - Min | Cardinality - Max | Data Type Mapping | Vocabulary Mapping (IS, ID, CE, CEN, CWE) | Assignment
1 | RPT.1 | Repeat Pattern Code | CWE | 1 | 1 |  |  |  | code |  | CodeableConcept | 0 | 1 |  | RepeatPattern |  |
2 | RPT.2 | Calendar Alignment | ID | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
3 | RPT.3 | Phase Range Begin Value | NM | 0 | 1 | IF RPT.2 = "DW" |  |  | Timing.repeat.dayOfWeek |  | code | 0 | 1 |  |  | /translate number to day/ |
4 | RPT.4 | Phase Range End Value | NM | 0 | 1 | IF RPT.2 = "DW" |  |  | Timing.repeat.dayOfWeek |  | code | 0 | 1 |  |  | /translate number to day/ |
5 | RPT.5 | Period Quantity | NM | 0 | 1 |  |  |  | Timing.repeat.period |  | decimal | 0 | 1 |  |  |  |
6 | RPT.6 | Period Units | CWE | 0 | 1 |  |  |  | Timing.repeat.periodUnit |  | code | 0 | 1 |  |  |  |
7 | RPT.7 | Institution Specified Time | ID | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
8 | RPT.8 | Event | ID | 0 | 1 |  |  |  | Timing.repeat.when |  | code | 0 | 1 |  | EventRelatedPeriod |  |
9 | RPT.9 | Event Offset Quantity | NM | 0 | 1 |  |  |  | Timing.repeat.offset |  | unsignedInt | 0 | 1 |  |  | /convert to minutes based on RPT.10/ |
10 | RPT.10 | Event Offset Units | CWE | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |
11 | RPT.11 | General Timing Specification | GTS | 0 | 1 |  |  |  |  |  |  |  |  |  |  |  |

Mapping from (not specified) to (not specified)

Group 1 Mapping from `unspecified code system` to `unspecified code system`

Source Concept Details | Relationship | Target Concept Details
Codes from | ComputableANTLR |  | Codes from
RPT.1 | Repeat Pattern Code |  | is equivalent to | code | code
RPT.3 | Phase Range Begin Value | IF RPT.2 = "DW" | is equivalent to | repeat.dayOfWeek[1] | repeat.dayOfWeek[1]
RPT.4 | Phase Range End Value | IF RPT.2 = "DW" | is equivalent to | repeat.dayOfWeek[2] | repeat.dayOfWeek[2]
RPT.5 | Period Quantity |  | is equivalent to | repeat.period | repeat.period
RPT.6 | Period Units |  | is equivalent to | repeat.periodUnit | repeat.periodUnit
RPT.8 | Event |  | is equivalent to | repeat.when | repeat.when
RPT.9 | Event Offset Quantity |  | is equivalent to | repeat.offset | repeat.offset

### Notes: