Personal Health Device Implementation Guide
1.0.0 - STU 1

Publication Build: This will be filled in by the publication tooling

## : Example of a Gateway - JSON Representation

Raw json | Download

    {
      "resourceType" : "Device",
      "id" : "phg-ecde3d4e58532d31.000000000000",
      "meta" : {
        "profile" : [
          "http://hl7.org/fhir/uv/phd/StructureDefinition/PhgDevice"
        ]
      },
      "text" : {
        "status" : "generated",
        "div" : "<div xmlns=\"http://www.w3.org/1999/xhtml\"><p><b>Generated Narrative</b></p><div style=\"display: inline-block; background-color: #d9e0e7; padding: 6px; margin: 4px; border: 1px solid #8da1b4; border-radius: 5px; line-height: 60%\"><p style=\"margin-bottom: 0px\">Resource \"phg-ecde3d4e58532d31.000000000000\" </p><p style=\"margin-bottom: 0px\">Profile: <a href=\"StructureDefinition-PhgDevice.html\">PhgDevice</a></p></div><p><b>identifier</b>: IEEE 11073 System Identifier: ec-de-3d-4e-58-53-2d-31, Bluetooth MAC address: 3d-4e-58-53-2d-31, Ethernet MAC address: 3d-4e-58-53-2d-35</p><p><b>type</b>: MDC_MOC_VMS_MDS_AHD <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#531981)</span></p><h3>Versions</h3><table class=\"grid\"><tr><td>-</td><td><b>Type</b></td><td><b>Value</b></td></tr><tr><td>*</td><td>MDC_REG_CERT_DATA_CONTINUA_VERSION: Continua version <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#532352)</span></td><td>5.0</td></tr></table><blockquote><p><b>property</b></p><p><b>type</b>: MDC_TIME_SYNC_PROTOCOL: Time synchronization protocol <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#68220)</span></p><p><b>valueCode</b>: MDC_TIME_SYNC_NTPV4: <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#532226)</span></p></blockquote><blockquote><p><b>property</b></p><p><b>type</b>: MDC_REG_CERT_DATA_CONTINUA_CERT_DEV_LIST: certified device list as transport-specialization combo <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#532353)</span></p><p><b>valueCode</b>: Pulse Oximeter certified <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"CodeSystem-ContinuaPHD.html\">ContinuaPHD</a>#4)</span></p></blockquote><blockquote><p><b>property</b></p><p><b>type</b>: MDC_REG_CERT_DATA_CONTINUA_AHD_CERT_LIST: certified Upload classes <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://terminology.hl7.org/3.1.0/CodeSystem-v3-mdc.html\">ISO 11073-10101 Health informatics - Point-of-care</a>#532355)</span></p><p><b>valueCode</b>: observation-upload-soap <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"CodeSystem-ContinuaHFS.html\">ContinuaHFS</a>#0)</span>, observation-upload-hdata <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"CodeSystem-ContinuaHFS.html\">ContinuaHFS</a>#3)</span>, observation-upload-fhir <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"CodeSystem-ContinuaHFS.html\">ContinuaHFS</a>#7)</span>, capabilities <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"CodeSystem-ContinuaHFS.html\">ContinuaHFS</a>#2)</span>, aps <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"CodeSystem-ContinuaHFS.html\">ContinuaHFS</a>#6)</span></p></blockquote><blockquote><p><b>property</b></p><p><b>type</b>: regulation-status <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"CodeSystem-ASN1ToHL7.html\">ASN1ToHL7</a>#532354.0)</span></p><p><b>valueCode</b>: Device is not regulated <span style=\"background: LightGoldenRodYellow; margin: 4px; border: 1px solid khaki\"> (<a href=\"http://hl7.org/fhir/R4/v2/0136/index.html\">v2 Y/N Indicator</a>#Y)</span></p></blockquote></div>"
      },
      "identifier" : [
        {
          "type" : {
            "coding" : [
              {
                "system" : "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers",
                "code" : "SYSID"
              }
            ]
          },
          "system" : "urn:oid:1.2.840.10004.1.1.1.0.0.1.0.0.1.2680",
          "value" : "ec-de-3d-4e-58-53-2d-31"
        },
        {
          "type" : {
            "coding" : [
              {
                "system" : "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers",
                "code" : "BTMAC"
              }
            ]
          },
          "system" : "http://hl7.org/fhir/sid/eui-48/bluetooth",
          "value" : "3d-4e-58-53-2d-31"
        },
        {
          "type" : {
            "coding" : [
              {
                "system" : "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaDeviceIdentifiers",
                "code" : "ETHMAC"
              }
            ]
          },
          "system" : "http://hl7.org/fhir/sid/eui-48/ethernet",
          "value" : "3d-4e-58-53-2d-35"
        }
      ],
      "type" : {
        "coding" : [
          {
            "system" : "urn:iso:std:iso:11073:10101",
            "code" : "531981"
          }
        ],
        "text" : "MDC_MOC_VMS_MDS_AHD"
      },
      "version" : [
        {
          "type" : {
            "coding" : [
              {
                "system" : "urn:iso:std:iso:11073:10101",
                "code" : "532352"
              }
            ],
            "text" : "MDC_REG_CERT_DATA_CONTINUA_VERSION: Continua version"
          },
          "value" : "5.0"
        }
      ],
      "property" : [
        {
          "type" : {
            "coding" : [
              {
                "system" : "urn:iso:std:iso:11073:10101",
                "code" : "68220"
              }
            ],
            "text" : "MDC_TIME_SYNC_PROTOCOL: Time synchronization protocol"
          },
          "valueCode" : [
            {
              "coding" : [
                {
                  "system" : "urn:iso:std:iso:11073:10101",
                  "code" : "532226"
                }
              ],
              "text" : "MDC_TIME_SYNC_NTPV4:"
            }
          ]
        },
        {
          "type" : {
            "coding" : [
              {
                "system" : "urn:iso:std:iso:11073:10101",
                "code" : "532353"
              }
            ],
            "text" : "MDC_REG_CERT_DATA_CONTINUA_CERT_DEV_LIST: certified device list as transport-specialization combo"
          },
          "valueCode" : [
            {
              "coding" : [
                {
                  "system" : "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaPHD",
                  "code" : "4"
                }
              ]
            }
          ]
        },
        {
          "type" : {
            "coding" : [
              {
                "system" : "urn:iso:std:iso:11073:10101",
                "code" : "532355"
              }
            ],
            "text" : "MDC_REG_CERT_DATA_CONTINUA_AHD_CERT_LIST: certified Upload classes"
          },
          "valueCode" : [
            {
              "coding" : [
                {
                  "system" : "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaHFS",
                  "code" : "0"
                }
              ]
            },
            {
              "coding" : [
                {
                  "system" : "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaHFS",
                  "code" : "3"
                }
              ]
            },
            {
              "coding" : [
                {
                  "system" : "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaHFS",
                  "code" : "7"
                }
              ]
            },
            {
              "coding" : [
                {
                  "system" : "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaHFS",
                  "code" : "2"
                }
              ]
            },
            {
              "coding" : [
                {
                  "system" : "http://hl7.org/fhir/uv/phd/CodeSystem/ContinuaHFS",
                  "code" : "6"
                }
              ]
            }
          ]
        },
        {
          "type" : {
            "coding" : [
              {
                "system" : "http://hl7.org/fhir/uv/phd/CodeSystem/ASN1ToHL7",
                "code" : "532354.0"
              }
            ],
            "text" : "regulation-status"
          },
          "valueCode" : [
            {
              "coding" : [
                {
                  "system" : "http://terminology.hl7.org/CodeSystem/v2-0136",
                  "code" : "Y"
                }
              ],
              "text" : "Device is not regulated"
            }
          ]
        }
      ]
    }